\doxysection{include/osmocom/core/gsmtap.h File Reference}
\label{gsmtap_8h}\index{include/osmocom/core/gsmtap.h@{include/osmocom/core/gsmtap.h}}


gsmtap header, pseudo-\/header in front of the actua GSM payload.  


{\ttfamily \#include $<$stdint.\+h$>$}\newline
\doxysubsection*{Data Structures}
\begin{DoxyCompactItemize}
\item 
struct \textbf{ gsmtap\+\_\+hdr}
\begin{DoxyCompactList}\small\item\em Structure of the GSMTAP pseudo-\/header. \end{DoxyCompactList}\item 
struct \textbf{ gsmtap\+\_\+osmocore\+\_\+log\+\_\+hdr}
\begin{DoxyCompactList}\small\item\em Structure of the GSMTAP libosmocore logging header. \end{DoxyCompactList}\end{DoxyCompactItemize}
\doxysubsection*{Macros}
\begin{DoxyCompactItemize}
\item 
\#define \textbf{ GSMTAP\+\_\+\+VERSION}~0x02
\item 
\#define \textbf{ GSMTAP\+\_\+\+TYPE\+\_\+\+UM}~0x01
\item 
\#define \textbf{ GSMTAP\+\_\+\+TYPE\+\_\+\+ABIS}~0x02
\item 
\#define \textbf{ GSMTAP\+\_\+\+TYPE\+\_\+\+UM\+\_\+\+BURST}~0x03 /$\ast$ raw burst bits $\ast$/
\item 
\#define \textbf{ GSMTAP\+\_\+\+TYPE\+\_\+\+SIM}~0x04 /$\ast$ ISO 7816 smart card interface $\ast$/
\item 
\#define \textbf{ GSMTAP\+\_\+\+TYPE\+\_\+\+TETRA\+\_\+\+I1}~0x05 /$\ast$ tetra air interface $\ast$/
\item 
\#define \textbf{ GSMTAP\+\_\+\+TYPE\+\_\+\+TETRA\+\_\+\+I1\+\_\+\+BURST}~0x06 /$\ast$ tetra air interface $\ast$/
\item 
\#define \textbf{ GSMTAP\+\_\+\+TYPE\+\_\+\+WMX\+\_\+\+BURST}~0x07    /$\ast$ Wi\+MAX burst $\ast$/
\item 
\#define \textbf{ GSMTAP\+\_\+\+TYPE\+\_\+\+GB\+\_\+\+LLC}~0x08 /$\ast$ GPRS Gb interface\+: LLC $\ast$/
\item 
\#define \textbf{ GSMTAP\+\_\+\+TYPE\+\_\+\+GB\+\_\+\+SNDCP}~0x09 /$\ast$ GPRS Gb interface\+: SNDCP $\ast$/
\item 
\#define \textbf{ GSMTAP\+\_\+\+TYPE\+\_\+\+GMR1\+\_\+\+UM}~0x0a /$\ast$ GMR-\/1 L2 packets $\ast$/
\item 
\#define \textbf{ GSMTAP\+\_\+\+TYPE\+\_\+\+UMTS\+\_\+\+RLC\+\_\+\+MAC}~0x0b
\item 
\#define \textbf{ GSMTAP\+\_\+\+TYPE\+\_\+\+UMTS\+\_\+\+RRC}~0x0c
\item 
\#define \textbf{ GSMTAP\+\_\+\+TYPE\+\_\+\+LTE\+\_\+\+RRC}~0x0d /$\ast$ LTE interface $\ast$/
\item 
\#define \textbf{ GSMTAP\+\_\+\+TYPE\+\_\+\+LTE\+\_\+\+MAC}~0x0e /$\ast$ LTE MAC interface $\ast$/
\item 
\#define \textbf{ GSMTAP\+\_\+\+TYPE\+\_\+\+LTE\+\_\+\+MAC\+\_\+\+FRAMED}~0x0f /$\ast$ LTE MAC with context \textbf{ hdr} $\ast$/
\item 
\#define \textbf{ GSMTAP\+\_\+\+TYPE\+\_\+\+OSMOCORE\+\_\+\+LOG}~0x10 /$\ast$ \textbf{ libosmocore} logging $\ast$/
\item 
\#define \textbf{ GSMTAP\+\_\+\+TYPE\+\_\+\+QC\+\_\+\+DIAG}~0x11 /$\ast$ Qualcomm DIAG frame $\ast$/
\item 
\#define \textbf{ GSMTAP\+\_\+\+TYPE\+\_\+\+LTE\+\_\+\+NAS}~0x12 /$\ast$ LTE Non-\/Access Stratum $\ast$/
\item 
\#define \textbf{ GSMTAP\+\_\+\+TYPE\+\_\+\+E1\+T1}~0x13 /$\ast$ E1/\textbf{ T1} Lines $\ast$/
\item 
\#define \textbf{ GSMTAP\+\_\+\+TYPE\+\_\+\+GSM\+\_\+\+RLP}~0x14 /$\ast$ GSM RLP frames as per 3GPP TS 24.\+022 $\ast$/
\item 
\#define \textbf{ GSMTAP\+\_\+\+BURST\+\_\+\+UNKNOWN}~0x00
\item 
\#define \textbf{ GSMTAP\+\_\+\+BURST\+\_\+\+FCCH}~0x01
\item 
\#define \textbf{ GSMTAP\+\_\+\+BURST\+\_\+\+PARTIAL\+\_\+\+SCH}~0x02
\item 
\#define \textbf{ GSMTAP\+\_\+\+BURST\+\_\+\+SCH}~0x03
\item 
\#define \textbf{ GSMTAP\+\_\+\+BURST\+\_\+\+CTS\+\_\+\+SCH}~0x04
\item 
\#define \textbf{ GSMTAP\+\_\+\+BURST\+\_\+\+COMPACT\+\_\+\+SCH}~0x05
\item 
\#define \textbf{ GSMTAP\+\_\+\+BURST\+\_\+\+NORMAL}~0x06
\item 
\#define \textbf{ GSMTAP\+\_\+\+BURST\+\_\+\+DUMMY}~0x07
\item 
\#define \textbf{ GSMTAP\+\_\+\+BURST\+\_\+\+ACCESS}~0x08
\item 
\#define \textbf{ GSMTAP\+\_\+\+BURST\+\_\+\+NONE}~0x09
\item 
\#define \textbf{ GSMTAP\+\_\+\+BURST\+\_\+\+CDMA\+\_\+\+CODE}~0x10 /$\ast$ Wi\+MAX CDMA Code Attribute burst $\ast$/
\item 
\#define \textbf{ GSMTAP\+\_\+\+BURST\+\_\+\+FCH}~0x11 /$\ast$ Wi\+MAX FCH burst $\ast$/
\item 
\#define \textbf{ GSMTAP\+\_\+\+BURST\+\_\+\+FFB}~0x12 /$\ast$ Wi\+MAX Fast Feedback burst $\ast$/
\item 
\#define \textbf{ GSMTAP\+\_\+\+BURST\+\_\+\+PDU}~0x13 /$\ast$ Wi\+MAX PDU burst $\ast$/
\item 
\#define \textbf{ GSMTAP\+\_\+\+BURST\+\_\+\+HACK}~0x14 /$\ast$ Wi\+MAX HARQ ACK burst $\ast$/
\item 
\#define \textbf{ GSMTAP\+\_\+\+BURST\+\_\+\+PHY\+\_\+\+ATTRIBUTES}~0x15 /$\ast$ Wi\+MAX PHY Attributes burst $\ast$/
\item 
\#define \textbf{ GSMTAP\+\_\+\+CHANNEL\+\_\+\+UNKNOWN}~0x00
\item 
\#define \textbf{ GSMTAP\+\_\+\+CHANNEL\+\_\+\+BCCH}~0x01
\item 
\#define \textbf{ GSMTAP\+\_\+\+CHANNEL\+\_\+\+CCCH}~0x02
\item 
\#define \textbf{ GSMTAP\+\_\+\+CHANNEL\+\_\+\+RACH}~0x03
\item 
\#define \textbf{ GSMTAP\+\_\+\+CHANNEL\+\_\+\+AGCH}~0x04
\item 
\#define \textbf{ GSMTAP\+\_\+\+CHANNEL\+\_\+\+PCH}~0x05
\item 
\#define \textbf{ GSMTAP\+\_\+\+CHANNEL\+\_\+\+SDCCH}~0x06
\item 
\#define \textbf{ GSMTAP\+\_\+\+CHANNEL\+\_\+\+SDCCH4}~0x07
\item 
\#define \textbf{ GSMTAP\+\_\+\+CHANNEL\+\_\+\+SDCCH8}~0x08
\item 
\#define \textbf{ GSMTAP\+\_\+\+CHANNEL\+\_\+\+FACCH\+\_\+F}~0x09 /$\ast$ Actually, it\textquotesingle{}s FACCH/\textbf{ F} (signaling) $\ast$/
\item 
\#define \textbf{ GSMTAP\+\_\+\+CHANNEL\+\_\+\+FACCH\+\_\+H}~0x0a /$\ast$ Actually, it\textquotesingle{}s FACCH/\textbf{ H} (signaling) $\ast$/
\item 
\#define \textbf{ GSMTAP\+\_\+\+CHANNEL\+\_\+\+PACCH}~0x0b
\item 
\#define \textbf{ GSMTAP\+\_\+\+CHANNEL\+\_\+\+CBCH52}~0x0c
\item 
\#define \textbf{ GSMTAP\+\_\+\+CHANNEL\+\_\+\+PDTCH}~0x0d
\item 
\#define \textbf{ GSMTAP\+\_\+\+CHANNEL\+\_\+\+PDCH}~\textbf{ GSMTAP\+\_\+\+CHANNEL\+\_\+\+PDTCH}
\item 
\#define \textbf{ GSMTAP\+\_\+\+CHANNEL\+\_\+\+PTCCH}~0x0e
\item 
\#define \textbf{ GSMTAP\+\_\+\+CHANNEL\+\_\+\+CBCH51}~0x0f
\item 
\#define \textbf{ GSMTAP\+\_\+\+CHANNEL\+\_\+\+VOICE\+\_\+F}~0x10 /$\ast$ voice codec payload (FR/EFR/AMR) $\ast$/
\item 
\#define \textbf{ GSMTAP\+\_\+\+CHANNEL\+\_\+\+VOICE\+\_\+H}~0x11 /$\ast$ voice codec payload (HR/AMR) $\ast$/
\item 
\#define \textbf{ GSMTAP\+\_\+\+CHANNEL\+\_\+\+TCH\+\_\+F}~\textbf{ GSMTAP\+\_\+\+CHANNEL\+\_\+\+FACCH\+\_\+F} /$\ast$ We used the wrong naming in 2008 when we were young $\ast$/
\item 
\#define \textbf{ GSMTAP\+\_\+\+CHANNEL\+\_\+\+TCH\+\_\+H}~\textbf{ GSMTAP\+\_\+\+CHANNEL\+\_\+\+FACCH\+\_\+H} /$\ast$ We used the wrong naming in 2008 when we were young $\ast$/
\item 
\#define \textbf{ GSMTAP\+\_\+\+GPRS\+\_\+\+CS\+\_\+\+BASE}~0x20
\item 
\#define \textbf{ GSMTAP\+\_\+\+GPRS\+\_\+\+CS}(N)~(\textbf{ GSMTAP\+\_\+\+GPRS\+\_\+\+CS\+\_\+\+BASE} + N)
\item 
\#define \textbf{ GSMTAP\+\_\+\+GPRS\+\_\+\+MCS\+\_\+\+BASE}~0x30
\item 
\#define \textbf{ GSMTAP\+\_\+\+GPRS\+\_\+\+MCS}(N)~(\textbf{ GSMTAP\+\_\+\+GPRS\+\_\+\+MCS\+\_\+\+BASE} + N)
\item 
\#define \textbf{ GSMTAP\+\_\+\+CHANNEL\+\_\+\+ACCH}~0x80
\item 
\#define \textbf{ GSMTAP\+\_\+\+SIM\+\_\+\+APDU}~0x00 /$\ast$ APDU \textbf{ data} (complete APDU) $\ast$/
\item 
\#define \textbf{ GSMTAP\+\_\+\+SIM\+\_\+\+ATR}~0x01 /$\ast$ card ATR \textbf{ data} $\ast$/
\item 
\#define \textbf{ GSMTAP\+\_\+\+SIM\+\_\+\+PPS\+\_\+\+REQ}~0x02 /$\ast$ PPS request \textbf{ data} $\ast$/
\item 
\#define \textbf{ GSMTAP\+\_\+\+SIM\+\_\+\+PPS\+\_\+\+RSP}~0x03 /$\ast$ PPS response \textbf{ data} $\ast$/
\item 
\#define \textbf{ GSMTAP\+\_\+\+SIM\+\_\+\+TPDU\+\_\+\+HDR}~0x04 /$\ast$ TPDU command \textbf{ header} $\ast$/
\item 
\#define \textbf{ GSMTAP\+\_\+\+SIM\+\_\+\+TPDU\+\_\+\+CMD}~0x05 /$\ast$ TPDU command body $\ast$/
\item 
\#define \textbf{ GSMTAP\+\_\+\+SIM\+\_\+\+TPDU\+\_\+\+RSP}~0x06 /$\ast$ TPDU response body $\ast$/
\item 
\#define \textbf{ GSMTAP\+\_\+\+SIM\+\_\+\+TPDU\+\_\+\+SW}~0x07 /$\ast$ TPDU response trailer $\ast$/
\item 
\#define \textbf{ GSMTAP\+\_\+\+TETRA\+\_\+\+BSCH}~0x01
\item 
\#define \textbf{ GSMTAP\+\_\+\+TETRA\+\_\+\+AACH}~0x02
\item 
\#define \textbf{ GSMTAP\+\_\+\+TETRA\+\_\+\+SCH\+\_\+\+HU}~0x03
\item 
\#define \textbf{ GSMTAP\+\_\+\+TETRA\+\_\+\+SCH\+\_\+\+HD}~0x04
\item 
\#define \textbf{ GSMTAP\+\_\+\+TETRA\+\_\+\+SCH\+\_\+F}~0x05
\item 
\#define \textbf{ GSMTAP\+\_\+\+TETRA\+\_\+\+BNCH}~0x06
\item 
\#define \textbf{ GSMTAP\+\_\+\+TETRA\+\_\+\+STCH}~0x07
\item 
\#define \textbf{ GSMTAP\+\_\+\+TETRA\+\_\+\+TCH\+\_\+F}~0x08
\item 
\#define \textbf{ GSMTAP\+\_\+\+TETRA\+\_\+\+DMO\+\_\+\+SCH\+\_\+S}~0x09
\item 
\#define \textbf{ GSMTAP\+\_\+\+TETRA\+\_\+\+DMO\+\_\+\+SCH\+\_\+H}~0x0a
\item 
\#define \textbf{ GSMTAP\+\_\+\+TETRA\+\_\+\+DMO\+\_\+\+SCH\+\_\+F}~0x0b
\item 
\#define \textbf{ GSMTAP\+\_\+\+TETRA\+\_\+\+DMO\+\_\+\+STCH}~0x0c
\item 
\#define \textbf{ GSMTAP\+\_\+\+TETRA\+\_\+\+DMO\+\_\+\+TCH}~0x0d
\item 
\#define \textbf{ GSMTAP\+\_\+\+GMR1\+\_\+\+UNKNOWN}~0x00
\item 
\#define \textbf{ GSMTAP\+\_\+\+GMR1\+\_\+\+BCCH}~0x01
\item 
\#define \textbf{ GSMTAP\+\_\+\+GMR1\+\_\+\+CCCH}~0x02 /$\ast$ either AGCH or PCH $\ast$/
\item 
\#define \textbf{ GSMTAP\+\_\+\+GMR1\+\_\+\+PCH}~0x03
\item 
\#define \textbf{ GSMTAP\+\_\+\+GMR1\+\_\+\+AGCH}~0x04
\item 
\#define \textbf{ GSMTAP\+\_\+\+GMR1\+\_\+\+BACH}~0x05
\item 
\#define \textbf{ GSMTAP\+\_\+\+GMR1\+\_\+\+RACH}~0x06
\item 
\#define \textbf{ GSMTAP\+\_\+\+GMR1\+\_\+\+CBCH}~0x07
\item 
\#define \textbf{ GSMTAP\+\_\+\+GMR1\+\_\+\+SDCCH}~0x08
\item 
\#define \textbf{ GSMTAP\+\_\+\+GMR1\+\_\+\+TACCH}~0x09
\item 
\#define \textbf{ GSMTAP\+\_\+\+GMR1\+\_\+\+GBCH}~0x0a
\item 
\#define \textbf{ GSMTAP\+\_\+\+GMR1\+\_\+\+SACCH}~0x01 /$\ast$ to be combined with \+\_\+\+TCH\{6,9\}   $\ast$/
\item 
\#define \textbf{ GSMTAP\+\_\+\+GMR1\+\_\+\+FACCH}~0x02 /$\ast$ to be combines with \+\_\+\+TCH\{3,6,9\} $\ast$/
\item 
\#define \textbf{ GSMTAP\+\_\+\+GMR1\+\_\+\+DKAB}~0x03 /$\ast$ to be combined with \+\_\+\+TCH3 $\ast$/
\item 
\#define \textbf{ GSMTAP\+\_\+\+GMR1\+\_\+\+TCH3}~0x10
\item 
\#define \textbf{ GSMTAP\+\_\+\+GMR1\+\_\+\+TCH6}~0x14
\item 
\#define \textbf{ GSMTAP\+\_\+\+GMR1\+\_\+\+TCH9}~0x18
\item 
\#define \textbf{ GSMTAP\+\_\+\+UMTS\+\_\+\+CH\+\_\+\+PCCH}~0x01
\item 
\#define \textbf{ GSMTAP\+\_\+\+UMTS\+\_\+\+CH\+\_\+\+CCCH}~0x02
\item 
\#define \textbf{ GSMTAP\+\_\+\+UMTS\+\_\+\+CH\+\_\+\+DCCH}~0x03
\item 
\#define \textbf{ GSMTAP\+\_\+\+LTE\+\_\+\+CH\+\_\+\+BCCH}~0x01
\item 
\#define \textbf{ GSMTAP\+\_\+\+LTE\+\_\+\+CH\+\_\+\+CCCH}~0x02
\item 
\#define \textbf{ GSMTAP\+\_\+\+LTE\+\_\+\+CH\+\_\+\+DCCH}~0x03
\item 
\#define \textbf{ GSMTAP\+\_\+\+LTE\+\_\+\+CH\+\_\+\+MCCH}~0x04
\item 
\#define \textbf{ GSMTAP\+\_\+\+LTE\+\_\+\+CH\+\_\+\+PCCH}~0x05
\item 
\#define \textbf{ GSMTAP\+\_\+\+LTE\+\_\+\+CH\+\_\+\+DTCH}~0x06
\item 
\#define \textbf{ GSMTAP\+\_\+\+LTE\+\_\+\+CH\+\_\+\+MTCH}~0x07
\item 
\#define \textbf{ GSMTAP\+\_\+\+E1\+T1\+\_\+\+LAPD}~0x01 /$\ast$ Q.\+921 LAPD $\ast$/
\item 
\#define \textbf{ GSMTAP\+\_\+\+E1\+T1\+\_\+\+FR}~0x02 /$\ast$ Frame Relay $\ast$/
\item 
\#define \textbf{ GSMTAP\+\_\+\+E1\+T1\+\_\+\+RAW}~0x03 /$\ast$ raw/transparent \textbf{ B}-\/channel $\ast$/
\item 
\#define \textbf{ GSMTAP\+\_\+\+E1\+T1\+\_\+\+TRAU16}~0x04 /$\ast$ 16\textbf{ k} TRAU frames; sub-\/slot 0-\/3 $\ast$/
\item 
\#define \textbf{ GSMTAP\+\_\+\+E1\+T1\+\_\+\+TRAU8}~0x05 /$\ast$ 8\textbf{ k} TRAU frames; sub-\/slot 0-\/7 $\ast$/
\item 
\#define \textbf{ GSMTAP\+\_\+\+E1\+T1\+\_\+\+V5\+EF}~0x06 /$\ast$ V5 Envelope Function $\ast$/
\item 
\#define \textbf{ GSMTAP\+\_\+\+E1\+T1\+\_\+\+X75}~0x07 /$\ast$ X.\+75 \textbf{ B}-\/channel \textbf{ data} $\ast$/
\item 
\#define \textbf{ GSMTAP\+\_\+\+E1\+T1\+\_\+\+V120}~0x08 /$\ast$ V.\+120 \textbf{ B}-\/channel \textbf{ data} $\ast$/
\item 
\#define \textbf{ GSMTAP\+\_\+\+E1\+T1\+\_\+\+V110}~0x09 /$\ast$ V.\+110 \textbf{ B}-\/channel \textbf{ data} $\ast$/
\item 
\#define \textbf{ GSMTAP\+\_\+\+E1\+T1\+\_\+\+H221}~0x0a /$\ast$ H.\+221 \textbf{ B}-\/channel \textbf{ data} $\ast$/
\item 
\#define \textbf{ GSMTAP\+\_\+\+E1\+T1\+\_\+\+PPP}~0x0b /$\ast$ PPP $\ast$/
\item 
\#define \textbf{ GSMTAP\+\_\+\+ARFCN\+\_\+\+F\+\_\+\+PCS}~0x8000
\item 
\#define \textbf{ GSMTAP\+\_\+\+ARFCN\+\_\+\+F\+\_\+\+UPLINK}~0x4000
\item 
\#define \textbf{ GSMTAP\+\_\+\+ARFCN\+\_\+\+MASK}~0x3fff
\item 
\#define \textbf{ GSMTAP\+\_\+\+UDP\+\_\+\+PORT}~4729
\end{DoxyCompactItemize}
\doxysubsection*{Enumerations}
\begin{DoxyCompactItemize}
\item 
enum \{ \newline
\textbf{ GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+DL\+\_\+\+DCCH\+\_\+\+Message} = 0
, \newline
\textbf{ GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+UL\+\_\+\+DCCH\+\_\+\+Message}
, \newline
\textbf{ GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+DL\+\_\+\+CCCH\+\_\+\+Message}
, \newline
\textbf{ GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+UL\+\_\+\+CCCH\+\_\+\+Message}
, \newline
\textbf{ GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+PCCH\+\_\+\+Message}
, \newline
\textbf{ GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+DL\+\_\+\+SHCCH\+\_\+\+Message}
, \newline
\textbf{ GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+UL\+\_\+\+SHCCH\+\_\+\+Message}
, \newline
\textbf{ GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+BCCH\+\_\+\+FACH\+\_\+\+Message}
, \newline
\textbf{ GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+BCCH\+\_\+\+BCH\+\_\+\+Message}
, \newline
\textbf{ GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+MCCH\+\_\+\+Message}
, \newline
\textbf{ GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+MSCH\+\_\+\+Message}
, \newline
\textbf{ GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Handover\+To\+UTRANCommand}
, \newline
\textbf{ GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Inter\+RATHandover\+Info}
, \newline
\textbf{ GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+System\+Information\+\_\+\+BCH}
, \newline
\textbf{ GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+System\+\_\+\+Information\+\_\+\+Container}
, \newline
\textbf{ GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+UE\+\_\+\+Radio\+Access\+Capability\+Info}
, \newline
\textbf{ GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Master\+Information\+Block}
, \newline
\textbf{ GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type1}
, \newline
\textbf{ GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type2}
, \newline
\textbf{ GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type3}
, \newline
\textbf{ GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type4}
, \newline
\textbf{ GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type5}
, \newline
\textbf{ GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type5bis}
, \newline
\textbf{ GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type6}
, \newline
\textbf{ GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type7}
, \newline
\textbf{ GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type8}
, \newline
\textbf{ GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type9}
, \newline
\textbf{ GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type10}
, \newline
\textbf{ GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type11}
, \newline
\textbf{ GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type11bis}
, \newline
\textbf{ GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type12}
, \newline
\textbf{ GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type13}
, \newline
\textbf{ GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type13\+\_\+1}
, \newline
\textbf{ GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type13\+\_\+2}
, \newline
\textbf{ GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type13\+\_\+3}
, \newline
\textbf{ GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type13\+\_\+4}
, \newline
\textbf{ GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type14}
, \newline
\textbf{ GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type15}
, \newline
\textbf{ GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type15bis}
, \newline
\textbf{ GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type15\+\_\+1}
, \newline
\textbf{ GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type15\+\_\+1bis}
, \newline
\textbf{ GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type15\+\_\+2}
, \newline
\textbf{ GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type15\+\_\+2bis}
, \newline
\textbf{ GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type15\+\_\+2ter}
, \newline
\textbf{ GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type15\+\_\+3}
, \newline
\textbf{ GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type15\+\_\+3bis}
, \newline
\textbf{ GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type15\+\_\+4}
, \newline
\textbf{ GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type15\+\_\+5}
, \newline
\textbf{ GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type15\+\_\+6}
, \newline
\textbf{ GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type15\+\_\+7}
, \newline
\textbf{ GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type15\+\_\+8}
, \newline
\textbf{ GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type16}
, \newline
\textbf{ GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type17}
, \newline
\textbf{ GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type18}
, \newline
\textbf{ GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type19}
, \newline
\textbf{ GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type20}
, \newline
\textbf{ GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type21}
, \newline
\textbf{ GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type22}
, \newline
\textbf{ GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type\+SB1}
, \newline
\textbf{ GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type\+SB2}
, \newline
\textbf{ GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+To\+Target\+RNC\+\_\+\+Container}
, \newline
\textbf{ GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Target\+RNC\+\_\+\+To\+Source\+RNC\+\_\+\+Container}
, \newline
\textbf{ GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+MAX}
 \}
\item 
enum \{ \newline
\textbf{ GSMTAP\+\_\+\+LTE\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+DL\+\_\+\+CCCH\+\_\+\+Message} = 0
, \newline
\textbf{ GSMTAP\+\_\+\+LTE\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+DL\+\_\+\+DCCH\+\_\+\+Message}
, \newline
\textbf{ GSMTAP\+\_\+\+LTE\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+UL\+\_\+\+CCCH\+\_\+\+Message}
, \newline
\textbf{ GSMTAP\+\_\+\+LTE\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+UL\+\_\+\+DCCH\+\_\+\+Message}
, \newline
\textbf{ GSMTAP\+\_\+\+LTE\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+BCCH\+\_\+\+BCH\+\_\+\+Message}
, \newline
\textbf{ GSMTAP\+\_\+\+LTE\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+BCCH\+\_\+\+DL\+\_\+\+SCH\+\_\+\+Message}
, \newline
\textbf{ GSMTAP\+\_\+\+LTE\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+PCCH\+\_\+\+Message}
, \newline
\textbf{ GSMTAP\+\_\+\+LTE\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+MCCH\+\_\+\+Message}
, \newline
\textbf{ GSMTAP\+\_\+\+LTE\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+BCCH\+\_\+\+BCH\+\_\+\+Message\+\_\+\+MBMS}
, \newline
\textbf{ GSMTAP\+\_\+\+LTE\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+BCCH\+\_\+\+DL\+\_\+\+SCH\+\_\+\+Message\+\_\+\+BR}
, \newline
\textbf{ GSMTAP\+\_\+\+LTE\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+BCCH\+\_\+\+DL\+\_\+\+SCH\+\_\+\+Message\+\_\+\+MBMS}
, \newline
\textbf{ GSMTAP\+\_\+\+LTE\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+SC\+\_\+\+MCCH\+\_\+\+Message}
, \newline
\textbf{ GSMTAP\+\_\+\+LTE\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+SBCCH\+\_\+\+SL\+\_\+\+BCH\+\_\+\+Message}
, \newline
\textbf{ GSMTAP\+\_\+\+LTE\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+SBCCH\+\_\+\+SL\+\_\+\+BCH\+\_\+\+Message\+\_\+\+V2X}
, \newline
\textbf{ GSMTAP\+\_\+\+LTE\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+DL\+\_\+\+CCCH\+\_\+\+Message\+\_\+\+NB}
, \newline
\textbf{ GSMTAP\+\_\+\+LTE\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+DL\+\_\+\+DCCH\+\_\+\+Message\+\_\+\+NB}
, \newline
\textbf{ GSMTAP\+\_\+\+LTE\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+UL\+\_\+\+CCCH\+\_\+\+Message\+\_\+\+NB}
, \newline
\textbf{ GSMTAP\+\_\+\+LTE\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+UL\+\_\+\+DCCH\+\_\+\+Message\+\_\+\+NB}
, \newline
\textbf{ GSMTAP\+\_\+\+LTE\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+BCCH\+\_\+\+BCH\+\_\+\+Message\+\_\+\+NB}
, \newline
\textbf{ GSMTAP\+\_\+\+LTE\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+BCCH\+\_\+\+BCH\+\_\+\+Message\+\_\+\+TDD\+\_\+\+NB}
, \newline
\textbf{ GSMTAP\+\_\+\+LTE\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+BCCH\+\_\+\+DL\+\_\+\+SCH\+\_\+\+Message\+\_\+\+NB}
, \newline
\textbf{ GSMTAP\+\_\+\+LTE\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+PCCH\+\_\+\+Message\+\_\+\+NB}
, \newline
\textbf{ GSMTAP\+\_\+\+LTE\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+SC\+\_\+\+MCCH\+\_\+\+Message\+\_\+\+NB}
, \newline
\textbf{ GSMTAP\+\_\+\+LTE\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+MAX}
 \}
\item 
enum \{ \newline
\textbf{ GSMTAP\+\_\+\+LTE\+\_\+\+NAS\+\_\+\+PLAIN} = 0
, \newline
\textbf{ GSMTAP\+\_\+\+LTE\+\_\+\+NAS\+\_\+\+SEC\+\_\+\+HEADER}
, \newline
\textbf{ GSMTAP\+\_\+\+LTE\+\_\+\+NAS\+\_\+\+SUB\+\_\+\+MAX}
 \}
\item 
enum \textbf{ gsmtap\+\_\+um\+\_\+voice\+\_\+type} \{ \newline
\textbf{ GSMTAP\+\_\+\+UM\+\_\+\+VOICE\+\_\+\+HR}
, \newline
\textbf{ GSMTAP\+\_\+\+UM\+\_\+\+VOICE\+\_\+\+FR}
, \newline
\textbf{ GSMTAP\+\_\+\+UM\+\_\+\+VOICE\+\_\+\+EFR}
, \newline
\textbf{ GSMTAP\+\_\+\+UM\+\_\+\+VOICE\+\_\+\+AMR}
, \newline
\textbf{ GSMTAP\+\_\+\+UM\+\_\+\+VOICE\+\_\+\+AMR\+\_\+\+SID\+\_\+\+BAD}
, \newline
\textbf{ GSMTAP\+\_\+\+UM\+\_\+\+VOICE\+\_\+\+AMR\+\_\+\+ONSET}
, \newline
\textbf{ GSMTAP\+\_\+\+UM\+\_\+\+VOICE\+\_\+\+AMR\+\_\+\+RATSCCH}
, \newline
\textbf{ GSMTAP\+\_\+\+UM\+\_\+\+VOICE\+\_\+\+AMR\+\_\+\+SID\+\_\+\+UPDATE\+\_\+\+INH}
, \newline
\textbf{ GSMTAP\+\_\+\+UM\+\_\+\+VOICE\+\_\+\+AMR\+\_\+\+SID\+\_\+\+FIRST\+\_\+\+P1}
, \newline
\textbf{ GSMTAP\+\_\+\+UM\+\_\+\+VOICE\+\_\+\+AMR\+\_\+\+SID\+\_\+\+FIRST\+\_\+\+P2}
, \newline
\textbf{ GSMTAP\+\_\+\+UM\+\_\+\+VOICE\+\_\+\+AMR\+\_\+\+SID\+\_\+\+FIRST\+\_\+\+INH}
, \newline
\textbf{ GSMTAP\+\_\+\+UM\+\_\+\+VOICE\+\_\+\+AMR\+\_\+\+RATSCCH\+\_\+\+MARKER}
, \newline
\textbf{ GSMTAP\+\_\+\+UM\+\_\+\+VOICE\+\_\+\+AMR\+\_\+\+RATSCCH\+\_\+\+DATA}
 \}
\begin{DoxyCompactList}\small\item\em First byte of type==GSMTAP\+\_\+\+TYPE\+\_\+\+UM sub\+\_\+type==GSMTAP\+\_\+\+CHANNEL\+\_\+\+VOICE payload. \end{DoxyCompactList}\end{DoxyCompactItemize}
\doxysubsection*{Functions}
\begin{DoxyCompactItemize}
\item 
struct \textbf{ gsmtap\+\_\+hdr} \textbf{ \+\_\+\+\_\+attribute\+\_\+\+\_\+} ((packed))
\end{DoxyCompactItemize}
\doxysubsection*{Variables}
\begin{DoxyCompactItemize}
\item 
uint8\+\_\+t \textbf{ version}
\begin{DoxyCompactList}\small\item\em version, set to 0x01 currently \end{DoxyCompactList}\item 
uint8\+\_\+t \textbf{ hdr\+\_\+len}
\begin{DoxyCompactList}\small\item\em length in number of 32bit words \end{DoxyCompactList}\item 
uint8\+\_\+t \textbf{ type}
\begin{DoxyCompactList}\small\item\em see GSMTAP\+\_\+\+TYPE\+\_\+$\ast$ \end{DoxyCompactList}\item 
uint8\+\_\+t \textbf{ timeslot}
\begin{DoxyCompactList}\small\item\em timeslot (0..7 on Um) \end{DoxyCompactList}\item 
uint16\+\_\+t \textbf{ arfcn}
\begin{DoxyCompactList}\small\item\em ARFCN (frequency) \end{DoxyCompactList}\item 
int8\+\_\+t \textbf{ signal\+\_\+dbm}
\begin{DoxyCompactList}\small\item\em signal level in d\+Bm \end{DoxyCompactList}\item 
int8\+\_\+t \textbf{ snr\+\_\+db}
\begin{DoxyCompactList}\small\item\em signal/noise ratio in dB \end{DoxyCompactList}\item 
uint32\+\_\+t \textbf{ frame\+\_\+number}
\begin{DoxyCompactList}\small\item\em GSM Frame Number (FN) \end{DoxyCompactList}\item 
uint8\+\_\+t \textbf{ sub\+\_\+type}
\begin{DoxyCompactList}\small\item\em Type of burst/channel, see above. \end{DoxyCompactList}\item 
uint8\+\_\+t \textbf{ antenna\+\_\+nr}
\begin{DoxyCompactList}\small\item\em Antenna Number. \end{DoxyCompactList}\item 
uint8\+\_\+t \textbf{ sub\+\_\+slot}
\begin{DoxyCompactList}\small\item\em sub-\/slot within timeslot \end{DoxyCompactList}\item 
uint8\+\_\+t \textbf{ res}
\begin{DoxyCompactList}\small\item\em reserved for future use (RFU) \end{DoxyCompactList}\item 
\begin{tabbing}
xx\=xx\=xx\=xx\=xx\=xx\=xx\=xx\=xx\=\kill
struct \{\\
\>uint32\_t \textbf{ sec}\\
\>uint32\_t \textbf{ usec}\\
\} \textbf{ ts}\\

\end{tabbing}\item 
char \textbf{ proc\+\_\+name} [16]
\begin{DoxyCompactList}\small\item\em name of process \end{DoxyCompactList}\item 
uint32\+\_\+t \textbf{ pid}
\begin{DoxyCompactList}\small\item\em process ID \end{DoxyCompactList}\item 
uint8\+\_\+t \textbf{ level}
\begin{DoxyCompactList}\small\item\em logging level \end{DoxyCompactList}\item 
uint8\+\_\+t \textbf{ \+\_\+pad} [3]
\item 
char \textbf{ subsys} [16]
\begin{DoxyCompactList}\small\item\em logging sub-\/system \end{DoxyCompactList}\item 
\begin{tabbing}
xx\=xx\=xx\=xx\=xx\=xx\=xx\=xx\=xx\=\kill
struct \{\\
\>char \textbf{ name} [32]\\
\>\>{\em source file name }\\
\>uint32\_t \textbf{ line\_nr}\\
\>\>{\em line number }\\
\} \textbf{ src\_file}\\

\end{tabbing}\item 
enum \textbf{ gsmtap\+\_\+um\+\_\+voice\+\_\+type} \textbf{ \+\_\+\+\_\+attribute\+\_\+\+\_\+}
\end{DoxyCompactItemize}


\doxysubsection{Detailed Description}
gsmtap header, pseudo-\/header in front of the actua GSM payload. 

GSMTAP is a generic header format for GSM protocol captures, it uses the IANA-\/assigned UDP port number 4729 and carries payload in various formats of GSM interfaces such as Um MAC blocks or Um bursts.

Example programs generating GSMTAP data are airprobe ({\texttt{ http\+://airprobe.\+org/}}) or Osmocom\+BB ({\texttt{ http\+://bb.\+osmocom.\+org/}}) 

\doxysubsection{Macro Definition Documentation}
\mbox{\label{gsmtap_8h_ab7816edfea9a9c1edd306c11eb3972fb}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_ARFCN\_F\_PCS@{GSMTAP\_ARFCN\_F\_PCS}}
\index{GSMTAP\_ARFCN\_F\_PCS@{GSMTAP\_ARFCN\_F\_PCS}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_ARFCN\_F\_PCS}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+ARFCN\+\_\+\+F\+\_\+\+PCS~0x8000}

\mbox{\label{gsmtap_8h_a18baf6e04e58b611c015652b9ecf30f8}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_ARFCN\_F\_UPLINK@{GSMTAP\_ARFCN\_F\_UPLINK}}
\index{GSMTAP\_ARFCN\_F\_UPLINK@{GSMTAP\_ARFCN\_F\_UPLINK}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_ARFCN\_F\_UPLINK}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+ARFCN\+\_\+\+F\+\_\+\+UPLINK~0x4000}

\mbox{\label{gsmtap_8h_a43ee543cd7e8a6e52b172b6a8c85251c}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_ARFCN\_MASK@{GSMTAP\_ARFCN\_MASK}}
\index{GSMTAP\_ARFCN\_MASK@{GSMTAP\_ARFCN\_MASK}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_ARFCN\_MASK}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+ARFCN\+\_\+\+MASK~0x3fff}

\mbox{\label{gsmtap_8h_a8d9e26d2c996cc21dbcbeb209babcabe}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_BURST\_ACCESS@{GSMTAP\_BURST\_ACCESS}}
\index{GSMTAP\_BURST\_ACCESS@{GSMTAP\_BURST\_ACCESS}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_BURST\_ACCESS}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+BURST\+\_\+\+ACCESS~0x08}

\mbox{\label{gsmtap_8h_a4248e68d6293784641a0028062ebd10f}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_BURST\_CDMA\_CODE@{GSMTAP\_BURST\_CDMA\_CODE}}
\index{GSMTAP\_BURST\_CDMA\_CODE@{GSMTAP\_BURST\_CDMA\_CODE}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_BURST\_CDMA\_CODE}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+BURST\+\_\+\+CDMA\+\_\+\+CODE~0x10 /$\ast$ Wi\+MAX CDMA Code Attribute burst $\ast$/}

\mbox{\label{gsmtap_8h_ac935538ae82fb76944d6125a484f26f7}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_BURST\_COMPACT\_SCH@{GSMTAP\_BURST\_COMPACT\_SCH}}
\index{GSMTAP\_BURST\_COMPACT\_SCH@{GSMTAP\_BURST\_COMPACT\_SCH}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_BURST\_COMPACT\_SCH}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+BURST\+\_\+\+COMPACT\+\_\+\+SCH~0x05}

\mbox{\label{gsmtap_8h_ae57f1b6a6fc857936b92e33a59d98cd5}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_BURST\_CTS\_SCH@{GSMTAP\_BURST\_CTS\_SCH}}
\index{GSMTAP\_BURST\_CTS\_SCH@{GSMTAP\_BURST\_CTS\_SCH}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_BURST\_CTS\_SCH}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+BURST\+\_\+\+CTS\+\_\+\+SCH~0x04}

\mbox{\label{gsmtap_8h_a0ce63511d04dfe292f6439b6edfc9ace}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_BURST\_DUMMY@{GSMTAP\_BURST\_DUMMY}}
\index{GSMTAP\_BURST\_DUMMY@{GSMTAP\_BURST\_DUMMY}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_BURST\_DUMMY}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+BURST\+\_\+\+DUMMY~0x07}

\mbox{\label{gsmtap_8h_a56c1fe8617ab45a7fb80624a69958850}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_BURST\_FCCH@{GSMTAP\_BURST\_FCCH}}
\index{GSMTAP\_BURST\_FCCH@{GSMTAP\_BURST\_FCCH}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_BURST\_FCCH}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+BURST\+\_\+\+FCCH~0x01}

\mbox{\label{gsmtap_8h_aaec85d3dec5db6991812ff8849c50c03}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_BURST\_FCH@{GSMTAP\_BURST\_FCH}}
\index{GSMTAP\_BURST\_FCH@{GSMTAP\_BURST\_FCH}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_BURST\_FCH}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+BURST\+\_\+\+FCH~0x11 /$\ast$ Wi\+MAX FCH burst $\ast$/}

\mbox{\label{gsmtap_8h_ab8e4fc2c62ddbd73fe58b2d27d0bdeaa}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_BURST\_FFB@{GSMTAP\_BURST\_FFB}}
\index{GSMTAP\_BURST\_FFB@{GSMTAP\_BURST\_FFB}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_BURST\_FFB}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+BURST\+\_\+\+FFB~0x12 /$\ast$ Wi\+MAX Fast Feedback burst $\ast$/}

\mbox{\label{gsmtap_8h_a35af5eb2ea462e8ef52b2b84b1f52746}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_BURST\_HACK@{GSMTAP\_BURST\_HACK}}
\index{GSMTAP\_BURST\_HACK@{GSMTAP\_BURST\_HACK}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_BURST\_HACK}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+BURST\+\_\+\+HACK~0x14 /$\ast$ Wi\+MAX HARQ ACK burst $\ast$/}

\mbox{\label{gsmtap_8h_a52935a9b345e4a92ed8bd95bbc184b27}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_BURST\_NONE@{GSMTAP\_BURST\_NONE}}
\index{GSMTAP\_BURST\_NONE@{GSMTAP\_BURST\_NONE}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_BURST\_NONE}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+BURST\+\_\+\+NONE~0x09}

\mbox{\label{gsmtap_8h_ae8c283db6042196863fa7f7bb215d97a}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_BURST\_NORMAL@{GSMTAP\_BURST\_NORMAL}}
\index{GSMTAP\_BURST\_NORMAL@{GSMTAP\_BURST\_NORMAL}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_BURST\_NORMAL}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+BURST\+\_\+\+NORMAL~0x06}

\mbox{\label{gsmtap_8h_af6467ac078ea19d16fd9cb24d3ecda7d}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_BURST\_PARTIAL\_SCH@{GSMTAP\_BURST\_PARTIAL\_SCH}}
\index{GSMTAP\_BURST\_PARTIAL\_SCH@{GSMTAP\_BURST\_PARTIAL\_SCH}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_BURST\_PARTIAL\_SCH}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+BURST\+\_\+\+PARTIAL\+\_\+\+SCH~0x02}

\mbox{\label{gsmtap_8h_ac64ebad3e2a008bcd3d6e818026e8bf3}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_BURST\_PDU@{GSMTAP\_BURST\_PDU}}
\index{GSMTAP\_BURST\_PDU@{GSMTAP\_BURST\_PDU}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_BURST\_PDU}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+BURST\+\_\+\+PDU~0x13 /$\ast$ Wi\+MAX PDU burst $\ast$/}

\mbox{\label{gsmtap_8h_a0f95b23aa09abdd673eb5398ca5039eb}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_BURST\_PHY\_ATTRIBUTES@{GSMTAP\_BURST\_PHY\_ATTRIBUTES}}
\index{GSMTAP\_BURST\_PHY\_ATTRIBUTES@{GSMTAP\_BURST\_PHY\_ATTRIBUTES}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_BURST\_PHY\_ATTRIBUTES}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+BURST\+\_\+\+PHY\+\_\+\+ATTRIBUTES~0x15 /$\ast$ Wi\+MAX PHY Attributes burst $\ast$/}

\mbox{\label{gsmtap_8h_a69386c56c0c4ab06b59f7ac8b3ed3507}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_BURST\_SCH@{GSMTAP\_BURST\_SCH}}
\index{GSMTAP\_BURST\_SCH@{GSMTAP\_BURST\_SCH}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_BURST\_SCH}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+BURST\+\_\+\+SCH~0x03}

\mbox{\label{gsmtap_8h_a029e8af211d1389fc7c75bc34b2469ea}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_BURST\_UNKNOWN@{GSMTAP\_BURST\_UNKNOWN}}
\index{GSMTAP\_BURST\_UNKNOWN@{GSMTAP\_BURST\_UNKNOWN}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_BURST\_UNKNOWN}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+BURST\+\_\+\+UNKNOWN~0x00}

\mbox{\label{gsmtap_8h_a24ac9973e10026f03f30e92edee90763}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_CHANNEL\_ACCH@{GSMTAP\_CHANNEL\_ACCH}}
\index{GSMTAP\_CHANNEL\_ACCH@{GSMTAP\_CHANNEL\_ACCH}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_CHANNEL\_ACCH}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+CHANNEL\+\_\+\+ACCH~0x80}

\mbox{\label{gsmtap_8h_afff02a97ce6cb7a353eb67870eded784}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_CHANNEL\_AGCH@{GSMTAP\_CHANNEL\_AGCH}}
\index{GSMTAP\_CHANNEL\_AGCH@{GSMTAP\_CHANNEL\_AGCH}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_CHANNEL\_AGCH}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+CHANNEL\+\_\+\+AGCH~0x04}

\mbox{\label{gsmtap_8h_ae48b5c2187eb9e3921a21800b2211e2c}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_CHANNEL\_BCCH@{GSMTAP\_CHANNEL\_BCCH}}
\index{GSMTAP\_CHANNEL\_BCCH@{GSMTAP\_CHANNEL\_BCCH}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_CHANNEL\_BCCH}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+CHANNEL\+\_\+\+BCCH~0x01}

\mbox{\label{gsmtap_8h_adda605c900649fc46d5d5db109828ee5}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_CHANNEL\_CBCH51@{GSMTAP\_CHANNEL\_CBCH51}}
\index{GSMTAP\_CHANNEL\_CBCH51@{GSMTAP\_CHANNEL\_CBCH51}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_CHANNEL\_CBCH51}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+CHANNEL\+\_\+\+CBCH51~0x0f}

\mbox{\label{gsmtap_8h_a67fe93aefe20a5d5db27cca63ba901a2}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_CHANNEL\_CBCH52@{GSMTAP\_CHANNEL\_CBCH52}}
\index{GSMTAP\_CHANNEL\_CBCH52@{GSMTAP\_CHANNEL\_CBCH52}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_CHANNEL\_CBCH52}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+CHANNEL\+\_\+\+CBCH52~0x0c}

\mbox{\label{gsmtap_8h_add3dc5a5af70f391df4758d4948014e6}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_CHANNEL\_CCCH@{GSMTAP\_CHANNEL\_CCCH}}
\index{GSMTAP\_CHANNEL\_CCCH@{GSMTAP\_CHANNEL\_CCCH}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_CHANNEL\_CCCH}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+CHANNEL\+\_\+\+CCCH~0x02}

\mbox{\label{gsmtap_8h_a9ae3eee25d9d5f0eaa9e0b903344a344}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_CHANNEL\_FACCH\_F@{GSMTAP\_CHANNEL\_FACCH\_F}}
\index{GSMTAP\_CHANNEL\_FACCH\_F@{GSMTAP\_CHANNEL\_FACCH\_F}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_CHANNEL\_FACCH\_F}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+CHANNEL\+\_\+\+FACCH\+\_\+F~0x09 /$\ast$ Actually, it\textquotesingle{}s FACCH/\textbf{ F} (signaling) $\ast$/}

\mbox{\label{gsmtap_8h_aea46edb2c9c6593db1354b44954d50c5}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_CHANNEL\_FACCH\_H@{GSMTAP\_CHANNEL\_FACCH\_H}}
\index{GSMTAP\_CHANNEL\_FACCH\_H@{GSMTAP\_CHANNEL\_FACCH\_H}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_CHANNEL\_FACCH\_H}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+CHANNEL\+\_\+\+FACCH\+\_\+H~0x0a /$\ast$ Actually, it\textquotesingle{}s FACCH/\textbf{ H} (signaling) $\ast$/}

\mbox{\label{gsmtap_8h_ae861fd8e077b82af469fbdf3dd507199}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_CHANNEL\_PACCH@{GSMTAP\_CHANNEL\_PACCH}}
\index{GSMTAP\_CHANNEL\_PACCH@{GSMTAP\_CHANNEL\_PACCH}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_CHANNEL\_PACCH}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+CHANNEL\+\_\+\+PACCH~0x0b}

\mbox{\label{gsmtap_8h_a86e3ed06a9965b34568828bbe7af1cbf}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_CHANNEL\_PCH@{GSMTAP\_CHANNEL\_PCH}}
\index{GSMTAP\_CHANNEL\_PCH@{GSMTAP\_CHANNEL\_PCH}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_CHANNEL\_PCH}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+CHANNEL\+\_\+\+PCH~0x05}

\mbox{\label{gsmtap_8h_ad6991e9a54f982cfbfe46701ba26384c}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_CHANNEL\_PDCH@{GSMTAP\_CHANNEL\_PDCH}}
\index{GSMTAP\_CHANNEL\_PDCH@{GSMTAP\_CHANNEL\_PDCH}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_CHANNEL\_PDCH}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+CHANNEL\+\_\+\+PDCH~\textbf{ GSMTAP\+\_\+\+CHANNEL\+\_\+\+PDTCH}}

\mbox{\label{gsmtap_8h_a9d59203296389054eed4231657de284a}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_CHANNEL\_PDTCH@{GSMTAP\_CHANNEL\_PDTCH}}
\index{GSMTAP\_CHANNEL\_PDTCH@{GSMTAP\_CHANNEL\_PDTCH}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_CHANNEL\_PDTCH}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+CHANNEL\+\_\+\+PDTCH~0x0d}

\mbox{\label{gsmtap_8h_ac2edc0119c86e163e5c186ad7fbc2c76}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_CHANNEL\_PTCCH@{GSMTAP\_CHANNEL\_PTCCH}}
\index{GSMTAP\_CHANNEL\_PTCCH@{GSMTAP\_CHANNEL\_PTCCH}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_CHANNEL\_PTCCH}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+CHANNEL\+\_\+\+PTCCH~0x0e}

\mbox{\label{gsmtap_8h_af9491d9327c33194b6bb33f98cf972d2}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_CHANNEL\_RACH@{GSMTAP\_CHANNEL\_RACH}}
\index{GSMTAP\_CHANNEL\_RACH@{GSMTAP\_CHANNEL\_RACH}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_CHANNEL\_RACH}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+CHANNEL\+\_\+\+RACH~0x03}

\mbox{\label{gsmtap_8h_a47e9516eeeba0e346cc270a6479496e4}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_CHANNEL\_SDCCH@{GSMTAP\_CHANNEL\_SDCCH}}
\index{GSMTAP\_CHANNEL\_SDCCH@{GSMTAP\_CHANNEL\_SDCCH}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_CHANNEL\_SDCCH}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+CHANNEL\+\_\+\+SDCCH~0x06}

\mbox{\label{gsmtap_8h_a5cff53337e31c55920f51b6e7e754449}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_CHANNEL\_SDCCH4@{GSMTAP\_CHANNEL\_SDCCH4}}
\index{GSMTAP\_CHANNEL\_SDCCH4@{GSMTAP\_CHANNEL\_SDCCH4}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_CHANNEL\_SDCCH4}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+CHANNEL\+\_\+\+SDCCH4~0x07}

\mbox{\label{gsmtap_8h_ab0ddec8cee59b3b93eaae47f1580fd56}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_CHANNEL\_SDCCH8@{GSMTAP\_CHANNEL\_SDCCH8}}
\index{GSMTAP\_CHANNEL\_SDCCH8@{GSMTAP\_CHANNEL\_SDCCH8}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_CHANNEL\_SDCCH8}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+CHANNEL\+\_\+\+SDCCH8~0x08}

\mbox{\label{gsmtap_8h_a6ecb9ead460a3d0b2876ce53e4e52f90}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_CHANNEL\_TCH\_F@{GSMTAP\_CHANNEL\_TCH\_F}}
\index{GSMTAP\_CHANNEL\_TCH\_F@{GSMTAP\_CHANNEL\_TCH\_F}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_CHANNEL\_TCH\_F}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+CHANNEL\+\_\+\+TCH\+\_\+F~\textbf{ GSMTAP\+\_\+\+CHANNEL\+\_\+\+FACCH\+\_\+F} /$\ast$ We used the wrong naming in 2008 when we were young $\ast$/}

\mbox{\label{gsmtap_8h_aa3ef8542bb907d1c386cdedfad8450df}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_CHANNEL\_TCH\_H@{GSMTAP\_CHANNEL\_TCH\_H}}
\index{GSMTAP\_CHANNEL\_TCH\_H@{GSMTAP\_CHANNEL\_TCH\_H}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_CHANNEL\_TCH\_H}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+CHANNEL\+\_\+\+TCH\+\_\+H~\textbf{ GSMTAP\+\_\+\+CHANNEL\+\_\+\+FACCH\+\_\+H} /$\ast$ We used the wrong naming in 2008 when we were young $\ast$/}

\mbox{\label{gsmtap_8h_aebbf577629abfe6558e42fee7802e21a}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_CHANNEL\_UNKNOWN@{GSMTAP\_CHANNEL\_UNKNOWN}}
\index{GSMTAP\_CHANNEL\_UNKNOWN@{GSMTAP\_CHANNEL\_UNKNOWN}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_CHANNEL\_UNKNOWN}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+CHANNEL\+\_\+\+UNKNOWN~0x00}

\mbox{\label{gsmtap_8h_a55ffedc96a9532a60cdcbefddbbfed83}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_CHANNEL\_VOICE\_F@{GSMTAP\_CHANNEL\_VOICE\_F}}
\index{GSMTAP\_CHANNEL\_VOICE\_F@{GSMTAP\_CHANNEL\_VOICE\_F}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_CHANNEL\_VOICE\_F}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+CHANNEL\+\_\+\+VOICE\+\_\+F~0x10 /$\ast$ voice codec payload (FR/EFR/AMR) $\ast$/}

\mbox{\label{gsmtap_8h_a26ae30f7436a704b46682308326908f9}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_CHANNEL\_VOICE\_H@{GSMTAP\_CHANNEL\_VOICE\_H}}
\index{GSMTAP\_CHANNEL\_VOICE\_H@{GSMTAP\_CHANNEL\_VOICE\_H}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_CHANNEL\_VOICE\_H}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+CHANNEL\+\_\+\+VOICE\+\_\+H~0x11 /$\ast$ voice codec payload (HR/AMR) $\ast$/}

\mbox{\label{gsmtap_8h_ad4dedcb459905cd2fabb2fa4803838ed}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_E1T1\_FR@{GSMTAP\_E1T1\_FR}}
\index{GSMTAP\_E1T1\_FR@{GSMTAP\_E1T1\_FR}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_E1T1\_FR}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+E1\+T1\+\_\+\+FR~0x02 /$\ast$ Frame Relay $\ast$/}

\mbox{\label{gsmtap_8h_a2b19eadcb2c80c1969fdb772af6d5eb1}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_E1T1\_H221@{GSMTAP\_E1T1\_H221}}
\index{GSMTAP\_E1T1\_H221@{GSMTAP\_E1T1\_H221}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_E1T1\_H221}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+E1\+T1\+\_\+\+H221~0x0a /$\ast$ H.\+221 \textbf{ B}-\/channel \textbf{ data} $\ast$/}

\mbox{\label{gsmtap_8h_a6171bb6ab16243ef4d4cfbd539836ec1}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_E1T1\_LAPD@{GSMTAP\_E1T1\_LAPD}}
\index{GSMTAP\_E1T1\_LAPD@{GSMTAP\_E1T1\_LAPD}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_E1T1\_LAPD}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+E1\+T1\+\_\+\+LAPD~0x01 /$\ast$ Q.\+921 LAPD $\ast$/}

\mbox{\label{gsmtap_8h_a64fdfe165866274b9a18e5c3b2da81eb}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_E1T1\_PPP@{GSMTAP\_E1T1\_PPP}}
\index{GSMTAP\_E1T1\_PPP@{GSMTAP\_E1T1\_PPP}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_E1T1\_PPP}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+E1\+T1\+\_\+\+PPP~0x0b /$\ast$ PPP $\ast$/}

\mbox{\label{gsmtap_8h_adeb9d1d18922c5177b4bc7eb7935371c}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_E1T1\_RAW@{GSMTAP\_E1T1\_RAW}}
\index{GSMTAP\_E1T1\_RAW@{GSMTAP\_E1T1\_RAW}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_E1T1\_RAW}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+E1\+T1\+\_\+\+RAW~0x03 /$\ast$ raw/transparent \textbf{ B}-\/channel $\ast$/}

\mbox{\label{gsmtap_8h_a525b27d8a220624ffd8b9740ae81eda9}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_E1T1\_TRAU16@{GSMTAP\_E1T1\_TRAU16}}
\index{GSMTAP\_E1T1\_TRAU16@{GSMTAP\_E1T1\_TRAU16}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_E1T1\_TRAU16}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+E1\+T1\+\_\+\+TRAU16~0x04 /$\ast$ 16\textbf{ k} TRAU frames; sub-\/slot 0-\/3 $\ast$/}

\mbox{\label{gsmtap_8h_af22c6e0bcc5edfb230c04562b6052b5f}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_E1T1\_TRAU8@{GSMTAP\_E1T1\_TRAU8}}
\index{GSMTAP\_E1T1\_TRAU8@{GSMTAP\_E1T1\_TRAU8}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_E1T1\_TRAU8}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+E1\+T1\+\_\+\+TRAU8~0x05 /$\ast$ 8\textbf{ k} TRAU frames; sub-\/slot 0-\/7 $\ast$/}

\mbox{\label{gsmtap_8h_aa4e4d32110b11893d3a1c3f82c6cb6b7}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_E1T1\_V110@{GSMTAP\_E1T1\_V110}}
\index{GSMTAP\_E1T1\_V110@{GSMTAP\_E1T1\_V110}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_E1T1\_V110}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+E1\+T1\+\_\+\+V110~0x09 /$\ast$ V.\+110 \textbf{ B}-\/channel \textbf{ data} $\ast$/}

\mbox{\label{gsmtap_8h_a1390bffefa1fcf8843712a831e2c8bfd}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_E1T1\_V120@{GSMTAP\_E1T1\_V120}}
\index{GSMTAP\_E1T1\_V120@{GSMTAP\_E1T1\_V120}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_E1T1\_V120}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+E1\+T1\+\_\+\+V120~0x08 /$\ast$ V.\+120 \textbf{ B}-\/channel \textbf{ data} $\ast$/}

\mbox{\label{gsmtap_8h_aaaf446f54f9311eb974f35b622c76014}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_E1T1\_V5EF@{GSMTAP\_E1T1\_V5EF}}
\index{GSMTAP\_E1T1\_V5EF@{GSMTAP\_E1T1\_V5EF}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_E1T1\_V5EF}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+E1\+T1\+\_\+\+V5\+EF~0x06 /$\ast$ V5 Envelope Function $\ast$/}

\mbox{\label{gsmtap_8h_a3fdfef2989ab9af47278cb564ac0f74e}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_E1T1\_X75@{GSMTAP\_E1T1\_X75}}
\index{GSMTAP\_E1T1\_X75@{GSMTAP\_E1T1\_X75}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_E1T1\_X75}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+E1\+T1\+\_\+\+X75~0x07 /$\ast$ X.\+75 \textbf{ B}-\/channel \textbf{ data} $\ast$/}

\mbox{\label{gsmtap_8h_adc49f2beca709d1e2981a6f9697d9706}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_GMR1\_AGCH@{GSMTAP\_GMR1\_AGCH}}
\index{GSMTAP\_GMR1\_AGCH@{GSMTAP\_GMR1\_AGCH}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_GMR1\_AGCH}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+GMR1\+\_\+\+AGCH~0x04}

\mbox{\label{gsmtap_8h_a3279c94fa11285a174aa3f535f8a3eb0}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_GMR1\_BACH@{GSMTAP\_GMR1\_BACH}}
\index{GSMTAP\_GMR1\_BACH@{GSMTAP\_GMR1\_BACH}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_GMR1\_BACH}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+GMR1\+\_\+\+BACH~0x05}

\mbox{\label{gsmtap_8h_a831495cfb3597d1be6c07a82395e8690}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_GMR1\_BCCH@{GSMTAP\_GMR1\_BCCH}}
\index{GSMTAP\_GMR1\_BCCH@{GSMTAP\_GMR1\_BCCH}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_GMR1\_BCCH}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+GMR1\+\_\+\+BCCH~0x01}

\mbox{\label{gsmtap_8h_abdf6d6ca4fa268c0ed88509879ddf8c1}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_GMR1\_CBCH@{GSMTAP\_GMR1\_CBCH}}
\index{GSMTAP\_GMR1\_CBCH@{GSMTAP\_GMR1\_CBCH}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_GMR1\_CBCH}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+GMR1\+\_\+\+CBCH~0x07}

\mbox{\label{gsmtap_8h_aae22c3b31d7d2637f1367ebc9e4e420c}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_GMR1\_CCCH@{GSMTAP\_GMR1\_CCCH}}
\index{GSMTAP\_GMR1\_CCCH@{GSMTAP\_GMR1\_CCCH}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_GMR1\_CCCH}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+GMR1\+\_\+\+CCCH~0x02 /$\ast$ either AGCH or PCH $\ast$/}

\mbox{\label{gsmtap_8h_a5321437b043fcc0d1afbed32137da79b}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_GMR1\_DKAB@{GSMTAP\_GMR1\_DKAB}}
\index{GSMTAP\_GMR1\_DKAB@{GSMTAP\_GMR1\_DKAB}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_GMR1\_DKAB}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+GMR1\+\_\+\+DKAB~0x03 /$\ast$ to be combined with \+\_\+\+TCH3 $\ast$/}

\mbox{\label{gsmtap_8h_a7d60fe12d8701251d1257b66c19d7ded}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_GMR1\_FACCH@{GSMTAP\_GMR1\_FACCH}}
\index{GSMTAP\_GMR1\_FACCH@{GSMTAP\_GMR1\_FACCH}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_GMR1\_FACCH}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+GMR1\+\_\+\+FACCH~0x02 /$\ast$ to be combines with \+\_\+\+TCH\{3,6,9\} $\ast$/}

\mbox{\label{gsmtap_8h_ad9caeea9444f565384d63dcdbbed771f}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_GMR1\_GBCH@{GSMTAP\_GMR1\_GBCH}}
\index{GSMTAP\_GMR1\_GBCH@{GSMTAP\_GMR1\_GBCH}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_GMR1\_GBCH}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+GMR1\+\_\+\+GBCH~0x0a}

\mbox{\label{gsmtap_8h_ae610004e9e485bb55aff5c6cc3e66af4}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_GMR1\_PCH@{GSMTAP\_GMR1\_PCH}}
\index{GSMTAP\_GMR1\_PCH@{GSMTAP\_GMR1\_PCH}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_GMR1\_PCH}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+GMR1\+\_\+\+PCH~0x03}

\mbox{\label{gsmtap_8h_aa54201f67c64e4287bb553bc113e1ddc}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_GMR1\_RACH@{GSMTAP\_GMR1\_RACH}}
\index{GSMTAP\_GMR1\_RACH@{GSMTAP\_GMR1\_RACH}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_GMR1\_RACH}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+GMR1\+\_\+\+RACH~0x06}

\mbox{\label{gsmtap_8h_ad8463933ee95b84c4d89ab58757b2d2e}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_GMR1\_SACCH@{GSMTAP\_GMR1\_SACCH}}
\index{GSMTAP\_GMR1\_SACCH@{GSMTAP\_GMR1\_SACCH}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_GMR1\_SACCH}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+GMR1\+\_\+\+SACCH~0x01 /$\ast$ to be combined with \+\_\+\+TCH\{6,9\}   $\ast$/}

\mbox{\label{gsmtap_8h_a6baef2e94a7c6c7c7bc450b3db585a9f}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_GMR1\_SDCCH@{GSMTAP\_GMR1\_SDCCH}}
\index{GSMTAP\_GMR1\_SDCCH@{GSMTAP\_GMR1\_SDCCH}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_GMR1\_SDCCH}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+GMR1\+\_\+\+SDCCH~0x08}

\mbox{\label{gsmtap_8h_acfe48055951f746fe65bb44d13c54e17}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_GMR1\_TACCH@{GSMTAP\_GMR1\_TACCH}}
\index{GSMTAP\_GMR1\_TACCH@{GSMTAP\_GMR1\_TACCH}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_GMR1\_TACCH}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+GMR1\+\_\+\+TACCH~0x09}

\mbox{\label{gsmtap_8h_a5f3c703c0c5c9d6d58076c03225efa56}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_GMR1\_TCH3@{GSMTAP\_GMR1\_TCH3}}
\index{GSMTAP\_GMR1\_TCH3@{GSMTAP\_GMR1\_TCH3}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_GMR1\_TCH3}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+GMR1\+\_\+\+TCH3~0x10}

\mbox{\label{gsmtap_8h_accdc219518c7bc30bb67674d3a23e2d3}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_GMR1\_TCH6@{GSMTAP\_GMR1\_TCH6}}
\index{GSMTAP\_GMR1\_TCH6@{GSMTAP\_GMR1\_TCH6}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_GMR1\_TCH6}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+GMR1\+\_\+\+TCH6~0x14}

\mbox{\label{gsmtap_8h_a6a43929153fbe5b0d3815e8409188b21}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_GMR1\_TCH9@{GSMTAP\_GMR1\_TCH9}}
\index{GSMTAP\_GMR1\_TCH9@{GSMTAP\_GMR1\_TCH9}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_GMR1\_TCH9}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+GMR1\+\_\+\+TCH9~0x18}

\mbox{\label{gsmtap_8h_ae924f816250aa914bca77545c03a1608}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_GMR1\_UNKNOWN@{GSMTAP\_GMR1\_UNKNOWN}}
\index{GSMTAP\_GMR1\_UNKNOWN@{GSMTAP\_GMR1\_UNKNOWN}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_GMR1\_UNKNOWN}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+GMR1\+\_\+\+UNKNOWN~0x00}

\mbox{\label{gsmtap_8h_a587e7eb5bb3d3ad6fc3a6b529bd81365}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_GPRS\_CS@{GSMTAP\_GPRS\_CS}}
\index{GSMTAP\_GPRS\_CS@{GSMTAP\_GPRS\_CS}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_GPRS\_CS}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+GPRS\+\_\+\+CS(\begin{DoxyParamCaption}\item[{}]{N }\end{DoxyParamCaption})~(\textbf{ GSMTAP\+\_\+\+GPRS\+\_\+\+CS\+\_\+\+BASE} + N)}

\mbox{\label{gsmtap_8h_a9a4fa54435edf621f1c61472807a35d8}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_GPRS\_CS\_BASE@{GSMTAP\_GPRS\_CS\_BASE}}
\index{GSMTAP\_GPRS\_CS\_BASE@{GSMTAP\_GPRS\_CS\_BASE}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_GPRS\_CS\_BASE}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+GPRS\+\_\+\+CS\+\_\+\+BASE~0x20}

\mbox{\label{gsmtap_8h_abfa536f50e62799675fa6224450bd0c2}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_GPRS\_MCS@{GSMTAP\_GPRS\_MCS}}
\index{GSMTAP\_GPRS\_MCS@{GSMTAP\_GPRS\_MCS}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_GPRS\_MCS}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+GPRS\+\_\+\+MCS(\begin{DoxyParamCaption}\item[{}]{N }\end{DoxyParamCaption})~(\textbf{ GSMTAP\+\_\+\+GPRS\+\_\+\+MCS\+\_\+\+BASE} + N)}

\mbox{\label{gsmtap_8h_add45a0716aed5683a1b7cf7edbaa2249}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_GPRS\_MCS\_BASE@{GSMTAP\_GPRS\_MCS\_BASE}}
\index{GSMTAP\_GPRS\_MCS\_BASE@{GSMTAP\_GPRS\_MCS\_BASE}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_GPRS\_MCS\_BASE}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+GPRS\+\_\+\+MCS\+\_\+\+BASE~0x30}

\mbox{\label{gsmtap_8h_aa39ccf1261106549e134c2b4545c25dc}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_LTE\_CH\_BCCH@{GSMTAP\_LTE\_CH\_BCCH}}
\index{GSMTAP\_LTE\_CH\_BCCH@{GSMTAP\_LTE\_CH\_BCCH}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_LTE\_CH\_BCCH}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+LTE\+\_\+\+CH\+\_\+\+BCCH~0x01}

\mbox{\label{gsmtap_8h_a9d8af5e68de9bd17671ca777021d0fbf}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_LTE\_CH\_CCCH@{GSMTAP\_LTE\_CH\_CCCH}}
\index{GSMTAP\_LTE\_CH\_CCCH@{GSMTAP\_LTE\_CH\_CCCH}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_LTE\_CH\_CCCH}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+LTE\+\_\+\+CH\+\_\+\+CCCH~0x02}

\mbox{\label{gsmtap_8h_ac1833218b1f6e29539ea66205c3ae8dc}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_LTE\_CH\_DCCH@{GSMTAP\_LTE\_CH\_DCCH}}
\index{GSMTAP\_LTE\_CH\_DCCH@{GSMTAP\_LTE\_CH\_DCCH}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_LTE\_CH\_DCCH}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+LTE\+\_\+\+CH\+\_\+\+DCCH~0x03}

\mbox{\label{gsmtap_8h_a5afef44245bb843390e6c4ef21cb88c9}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_LTE\_CH\_DTCH@{GSMTAP\_LTE\_CH\_DTCH}}
\index{GSMTAP\_LTE\_CH\_DTCH@{GSMTAP\_LTE\_CH\_DTCH}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_LTE\_CH\_DTCH}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+LTE\+\_\+\+CH\+\_\+\+DTCH~0x06}

\mbox{\label{gsmtap_8h_a6dcedd924627caa7027f82bdab3185e6}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_LTE\_CH\_MCCH@{GSMTAP\_LTE\_CH\_MCCH}}
\index{GSMTAP\_LTE\_CH\_MCCH@{GSMTAP\_LTE\_CH\_MCCH}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_LTE\_CH\_MCCH}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+LTE\+\_\+\+CH\+\_\+\+MCCH~0x04}

\mbox{\label{gsmtap_8h_a67c880784d3127d18127f9a42423652c}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_LTE\_CH\_MTCH@{GSMTAP\_LTE\_CH\_MTCH}}
\index{GSMTAP\_LTE\_CH\_MTCH@{GSMTAP\_LTE\_CH\_MTCH}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_LTE\_CH\_MTCH}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+LTE\+\_\+\+CH\+\_\+\+MTCH~0x07}

\mbox{\label{gsmtap_8h_a1f7477b7873738473fd2828006d24da7}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_LTE\_CH\_PCCH@{GSMTAP\_LTE\_CH\_PCCH}}
\index{GSMTAP\_LTE\_CH\_PCCH@{GSMTAP\_LTE\_CH\_PCCH}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_LTE\_CH\_PCCH}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+LTE\+\_\+\+CH\+\_\+\+PCCH~0x05}

\mbox{\label{gsmtap_8h_a9f660a6e81f948569fedd35c3ded9f33}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_SIM\_APDU@{GSMTAP\_SIM\_APDU}}
\index{GSMTAP\_SIM\_APDU@{GSMTAP\_SIM\_APDU}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_SIM\_APDU}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+SIM\+\_\+\+APDU~0x00 /$\ast$ APDU \textbf{ data} (complete APDU) $\ast$/}

\mbox{\label{gsmtap_8h_a67d1aaa986cbe5b4cd85eb6f48a38001}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_SIM\_ATR@{GSMTAP\_SIM\_ATR}}
\index{GSMTAP\_SIM\_ATR@{GSMTAP\_SIM\_ATR}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_SIM\_ATR}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+SIM\+\_\+\+ATR~0x01 /$\ast$ card ATR \textbf{ data} $\ast$/}

\mbox{\label{gsmtap_8h_a11e74cd1046b4d13b8f558ba075fa4df}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_SIM\_PPS\_REQ@{GSMTAP\_SIM\_PPS\_REQ}}
\index{GSMTAP\_SIM\_PPS\_REQ@{GSMTAP\_SIM\_PPS\_REQ}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_SIM\_PPS\_REQ}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+SIM\+\_\+\+PPS\+\_\+\+REQ~0x02 /$\ast$ PPS request \textbf{ data} $\ast$/}

\mbox{\label{gsmtap_8h_a666f842795b15be561bc65164dab22fc}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_SIM\_PPS\_RSP@{GSMTAP\_SIM\_PPS\_RSP}}
\index{GSMTAP\_SIM\_PPS\_RSP@{GSMTAP\_SIM\_PPS\_RSP}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_SIM\_PPS\_RSP}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+SIM\+\_\+\+PPS\+\_\+\+RSP~0x03 /$\ast$ PPS response \textbf{ data} $\ast$/}

\mbox{\label{gsmtap_8h_a4b96cb200b11f8e08135da0954a50a89}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_SIM\_TPDU\_CMD@{GSMTAP\_SIM\_TPDU\_CMD}}
\index{GSMTAP\_SIM\_TPDU\_CMD@{GSMTAP\_SIM\_TPDU\_CMD}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_SIM\_TPDU\_CMD}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+SIM\+\_\+\+TPDU\+\_\+\+CMD~0x05 /$\ast$ TPDU command body $\ast$/}

\mbox{\label{gsmtap_8h_ab13abdd43b29b93e642f16969164b592}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_SIM\_TPDU\_HDR@{GSMTAP\_SIM\_TPDU\_HDR}}
\index{GSMTAP\_SIM\_TPDU\_HDR@{GSMTAP\_SIM\_TPDU\_HDR}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_SIM\_TPDU\_HDR}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+SIM\+\_\+\+TPDU\+\_\+\+HDR~0x04 /$\ast$ TPDU command \textbf{ header} $\ast$/}

\mbox{\label{gsmtap_8h_a64090a2b3eb3a91f9789243accba1801}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_SIM\_TPDU\_RSP@{GSMTAP\_SIM\_TPDU\_RSP}}
\index{GSMTAP\_SIM\_TPDU\_RSP@{GSMTAP\_SIM\_TPDU\_RSP}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_SIM\_TPDU\_RSP}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+SIM\+\_\+\+TPDU\+\_\+\+RSP~0x06 /$\ast$ TPDU response body $\ast$/}

\mbox{\label{gsmtap_8h_aec4e3afaf091e22a3bd94cfd7b0c022a}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_SIM\_TPDU\_SW@{GSMTAP\_SIM\_TPDU\_SW}}
\index{GSMTAP\_SIM\_TPDU\_SW@{GSMTAP\_SIM\_TPDU\_SW}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_SIM\_TPDU\_SW}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+SIM\+\_\+\+TPDU\+\_\+\+SW~0x07 /$\ast$ TPDU response trailer $\ast$/}

\mbox{\label{gsmtap_8h_ad3ed40549145f475c7466ea84a7308d3}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_TETRA\_AACH@{GSMTAP\_TETRA\_AACH}}
\index{GSMTAP\_TETRA\_AACH@{GSMTAP\_TETRA\_AACH}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_TETRA\_AACH}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+TETRA\+\_\+\+AACH~0x02}

\mbox{\label{gsmtap_8h_a37a4ff6cb01fa5b56a21d786fafd5073}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_TETRA\_BNCH@{GSMTAP\_TETRA\_BNCH}}
\index{GSMTAP\_TETRA\_BNCH@{GSMTAP\_TETRA\_BNCH}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_TETRA\_BNCH}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+TETRA\+\_\+\+BNCH~0x06}

\mbox{\label{gsmtap_8h_a7259cdc729c701d10a3ddd3858c9a029}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_TETRA\_BSCH@{GSMTAP\_TETRA\_BSCH}}
\index{GSMTAP\_TETRA\_BSCH@{GSMTAP\_TETRA\_BSCH}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_TETRA\_BSCH}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+TETRA\+\_\+\+BSCH~0x01}

\mbox{\label{gsmtap_8h_a36060b61d6114265dae5e17ddaf52712}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_TETRA\_DMO\_SCH\_F@{GSMTAP\_TETRA\_DMO\_SCH\_F}}
\index{GSMTAP\_TETRA\_DMO\_SCH\_F@{GSMTAP\_TETRA\_DMO\_SCH\_F}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_TETRA\_DMO\_SCH\_F}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+TETRA\+\_\+\+DMO\+\_\+\+SCH\+\_\+F~0x0b}

\mbox{\label{gsmtap_8h_a9d718cbb25a12af3f3901327210d9471}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_TETRA\_DMO\_SCH\_H@{GSMTAP\_TETRA\_DMO\_SCH\_H}}
\index{GSMTAP\_TETRA\_DMO\_SCH\_H@{GSMTAP\_TETRA\_DMO\_SCH\_H}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_TETRA\_DMO\_SCH\_H}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+TETRA\+\_\+\+DMO\+\_\+\+SCH\+\_\+H~0x0a}

\mbox{\label{gsmtap_8h_a0577a44427d7454ab8210f9095aece82}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_TETRA\_DMO\_SCH\_S@{GSMTAP\_TETRA\_DMO\_SCH\_S}}
\index{GSMTAP\_TETRA\_DMO\_SCH\_S@{GSMTAP\_TETRA\_DMO\_SCH\_S}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_TETRA\_DMO\_SCH\_S}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+TETRA\+\_\+\+DMO\+\_\+\+SCH\+\_\+S~0x09}

\mbox{\label{gsmtap_8h_a37998b24f36352afd198d50ad9575f32}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_TETRA\_DMO\_STCH@{GSMTAP\_TETRA\_DMO\_STCH}}
\index{GSMTAP\_TETRA\_DMO\_STCH@{GSMTAP\_TETRA\_DMO\_STCH}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_TETRA\_DMO\_STCH}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+TETRA\+\_\+\+DMO\+\_\+\+STCH~0x0c}

\mbox{\label{gsmtap_8h_a7c8cc0fb56c394652145a1be4e2561c2}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_TETRA\_DMO\_TCH@{GSMTAP\_TETRA\_DMO\_TCH}}
\index{GSMTAP\_TETRA\_DMO\_TCH@{GSMTAP\_TETRA\_DMO\_TCH}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_TETRA\_DMO\_TCH}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+TETRA\+\_\+\+DMO\+\_\+\+TCH~0x0d}

\mbox{\label{gsmtap_8h_a881e268f3d32b14b95f090f1fc5fda2e}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_TETRA\_SCH\_F@{GSMTAP\_TETRA\_SCH\_F}}
\index{GSMTAP\_TETRA\_SCH\_F@{GSMTAP\_TETRA\_SCH\_F}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_TETRA\_SCH\_F}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+TETRA\+\_\+\+SCH\+\_\+F~0x05}

\mbox{\label{gsmtap_8h_a63c78de0b63c67c4cc93d5d6948296c8}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_TETRA\_SCH\_HD@{GSMTAP\_TETRA\_SCH\_HD}}
\index{GSMTAP\_TETRA\_SCH\_HD@{GSMTAP\_TETRA\_SCH\_HD}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_TETRA\_SCH\_HD}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+TETRA\+\_\+\+SCH\+\_\+\+HD~0x04}

\mbox{\label{gsmtap_8h_a84c0a112c354d67a9c08f068d103c9f4}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_TETRA\_SCH\_HU@{GSMTAP\_TETRA\_SCH\_HU}}
\index{GSMTAP\_TETRA\_SCH\_HU@{GSMTAP\_TETRA\_SCH\_HU}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_TETRA\_SCH\_HU}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+TETRA\+\_\+\+SCH\+\_\+\+HU~0x03}

\mbox{\label{gsmtap_8h_ade3dc16da7a1d696b5a145ffd7612df8}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_TETRA\_STCH@{GSMTAP\_TETRA\_STCH}}
\index{GSMTAP\_TETRA\_STCH@{GSMTAP\_TETRA\_STCH}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_TETRA\_STCH}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+TETRA\+\_\+\+STCH~0x07}

\mbox{\label{gsmtap_8h_ae1ff54e2813b70c303da3ba34b0a73ea}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_TETRA\_TCH\_F@{GSMTAP\_TETRA\_TCH\_F}}
\index{GSMTAP\_TETRA\_TCH\_F@{GSMTAP\_TETRA\_TCH\_F}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_TETRA\_TCH\_F}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+TETRA\+\_\+\+TCH\+\_\+F~0x08}

\mbox{\label{gsmtap_8h_a7de71fefaf7d797816cf4004356ceb19}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_TYPE\_ABIS@{GSMTAP\_TYPE\_ABIS}}
\index{GSMTAP\_TYPE\_ABIS@{GSMTAP\_TYPE\_ABIS}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_TYPE\_ABIS}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+TYPE\+\_\+\+ABIS~0x02}

\mbox{\label{gsmtap_8h_a873f988c8a9b49167197aec72f169099}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_TYPE\_E1T1@{GSMTAP\_TYPE\_E1T1}}
\index{GSMTAP\_TYPE\_E1T1@{GSMTAP\_TYPE\_E1T1}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_TYPE\_E1T1}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+TYPE\+\_\+\+E1\+T1~0x13 /$\ast$ E1/\textbf{ T1} Lines $\ast$/}

\mbox{\label{gsmtap_8h_a78a800fa49b63aff41c82c18f2547cbe}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_TYPE\_GB\_LLC@{GSMTAP\_TYPE\_GB\_LLC}}
\index{GSMTAP\_TYPE\_GB\_LLC@{GSMTAP\_TYPE\_GB\_LLC}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_TYPE\_GB\_LLC}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+TYPE\+\_\+\+GB\+\_\+\+LLC~0x08 /$\ast$ GPRS Gb interface\+: LLC $\ast$/}

\mbox{\label{gsmtap_8h_a7285990ef743c0f845ee1fdb1b5ca278}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_TYPE\_GB\_SNDCP@{GSMTAP\_TYPE\_GB\_SNDCP}}
\index{GSMTAP\_TYPE\_GB\_SNDCP@{GSMTAP\_TYPE\_GB\_SNDCP}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_TYPE\_GB\_SNDCP}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+TYPE\+\_\+\+GB\+\_\+\+SNDCP~0x09 /$\ast$ GPRS Gb interface\+: SNDCP $\ast$/}

\mbox{\label{gsmtap_8h_a93fd3c3da748c48ee9bd8753fb7537d2}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_TYPE\_GMR1\_UM@{GSMTAP\_TYPE\_GMR1\_UM}}
\index{GSMTAP\_TYPE\_GMR1\_UM@{GSMTAP\_TYPE\_GMR1\_UM}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_TYPE\_GMR1\_UM}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+TYPE\+\_\+\+GMR1\+\_\+\+UM~0x0a /$\ast$ GMR-\/1 L2 packets $\ast$/}

\mbox{\label{gsmtap_8h_ab1093cbd7fab8b81585d9202af96fc06}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_TYPE\_GSM\_RLP@{GSMTAP\_TYPE\_GSM\_RLP}}
\index{GSMTAP\_TYPE\_GSM\_RLP@{GSMTAP\_TYPE\_GSM\_RLP}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_TYPE\_GSM\_RLP}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+TYPE\+\_\+\+GSM\+\_\+\+RLP~0x14 /$\ast$ GSM RLP frames as per 3GPP TS 24.\+022 $\ast$/}

\mbox{\label{gsmtap_8h_af0d26b8483ea71528d920acec2d7192c}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_TYPE\_LTE\_MAC@{GSMTAP\_TYPE\_LTE\_MAC}}
\index{GSMTAP\_TYPE\_LTE\_MAC@{GSMTAP\_TYPE\_LTE\_MAC}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_TYPE\_LTE\_MAC}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+TYPE\+\_\+\+LTE\+\_\+\+MAC~0x0e /$\ast$ LTE MAC interface $\ast$/}

\mbox{\label{gsmtap_8h_a691d2cc38b387c357e71f1d6e814b283}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_TYPE\_LTE\_MAC\_FRAMED@{GSMTAP\_TYPE\_LTE\_MAC\_FRAMED}}
\index{GSMTAP\_TYPE\_LTE\_MAC\_FRAMED@{GSMTAP\_TYPE\_LTE\_MAC\_FRAMED}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_TYPE\_LTE\_MAC\_FRAMED}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+TYPE\+\_\+\+LTE\+\_\+\+MAC\+\_\+\+FRAMED~0x0f /$\ast$ LTE MAC with context \textbf{ hdr} $\ast$/}

\mbox{\label{gsmtap_8h_a6a7a7c17bd71ec8772ce6d271f8305c9}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_TYPE\_LTE\_NAS@{GSMTAP\_TYPE\_LTE\_NAS}}
\index{GSMTAP\_TYPE\_LTE\_NAS@{GSMTAP\_TYPE\_LTE\_NAS}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_TYPE\_LTE\_NAS}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+TYPE\+\_\+\+LTE\+\_\+\+NAS~0x12 /$\ast$ LTE Non-\/Access Stratum $\ast$/}

\mbox{\label{gsmtap_8h_ae9dad4f65b17506bc14f30c405702d81}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_TYPE\_LTE\_RRC@{GSMTAP\_TYPE\_LTE\_RRC}}
\index{GSMTAP\_TYPE\_LTE\_RRC@{GSMTAP\_TYPE\_LTE\_RRC}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_TYPE\_LTE\_RRC}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+TYPE\+\_\+\+LTE\+\_\+\+RRC~0x0d /$\ast$ LTE interface $\ast$/}

\mbox{\label{gsmtap_8h_a1bdc141d1b216f9d6e9f9e92283c5401}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_TYPE\_OSMOCORE\_LOG@{GSMTAP\_TYPE\_OSMOCORE\_LOG}}
\index{GSMTAP\_TYPE\_OSMOCORE\_LOG@{GSMTAP\_TYPE\_OSMOCORE\_LOG}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_TYPE\_OSMOCORE\_LOG}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+TYPE\+\_\+\+OSMOCORE\+\_\+\+LOG~0x10 /$\ast$ \textbf{ libosmocore} logging $\ast$/}

\mbox{\label{gsmtap_8h_ac857ba3a2f81c0649a1eeea4a47463fe}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_TYPE\_QC\_DIAG@{GSMTAP\_TYPE\_QC\_DIAG}}
\index{GSMTAP\_TYPE\_QC\_DIAG@{GSMTAP\_TYPE\_QC\_DIAG}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_TYPE\_QC\_DIAG}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+TYPE\+\_\+\+QC\+\_\+\+DIAG~0x11 /$\ast$ Qualcomm DIAG frame $\ast$/}

\mbox{\label{gsmtap_8h_a5d1d6ef387ae1f74f8176e6aa4879bbd}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_TYPE\_SIM@{GSMTAP\_TYPE\_SIM}}
\index{GSMTAP\_TYPE\_SIM@{GSMTAP\_TYPE\_SIM}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_TYPE\_SIM}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+TYPE\+\_\+\+SIM~0x04 /$\ast$ ISO 7816 smart card interface $\ast$/}

\mbox{\label{gsmtap_8h_a11f29f3a373147eab6a91ee0addd427a}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_TYPE\_TETRA\_I1@{GSMTAP\_TYPE\_TETRA\_I1}}
\index{GSMTAP\_TYPE\_TETRA\_I1@{GSMTAP\_TYPE\_TETRA\_I1}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_TYPE\_TETRA\_I1}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+TYPE\+\_\+\+TETRA\+\_\+\+I1~0x05 /$\ast$ tetra air interface $\ast$/}

\mbox{\label{gsmtap_8h_a50a93d09f323719926989d8332110d18}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_TYPE\_TETRA\_I1\_BURST@{GSMTAP\_TYPE\_TETRA\_I1\_BURST}}
\index{GSMTAP\_TYPE\_TETRA\_I1\_BURST@{GSMTAP\_TYPE\_TETRA\_I1\_BURST}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_TYPE\_TETRA\_I1\_BURST}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+TYPE\+\_\+\+TETRA\+\_\+\+I1\+\_\+\+BURST~0x06 /$\ast$ tetra air interface $\ast$/}

\mbox{\label{gsmtap_8h_acf35119501d58a6d15d0d3583d8914f4}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_TYPE\_UM@{GSMTAP\_TYPE\_UM}}
\index{GSMTAP\_TYPE\_UM@{GSMTAP\_TYPE\_UM}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_TYPE\_UM}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+TYPE\+\_\+\+UM~0x01}

\mbox{\label{gsmtap_8h_aa0f4415c48b0fd81572661b04463544d}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_TYPE\_UM\_BURST@{GSMTAP\_TYPE\_UM\_BURST}}
\index{GSMTAP\_TYPE\_UM\_BURST@{GSMTAP\_TYPE\_UM\_BURST}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_TYPE\_UM\_BURST}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+TYPE\+\_\+\+UM\+\_\+\+BURST~0x03 /$\ast$ raw burst bits $\ast$/}

\mbox{\label{gsmtap_8h_a5189ad680891d60cb12aab7ed1d78bf8}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_TYPE\_UMTS\_RLC\_MAC@{GSMTAP\_TYPE\_UMTS\_RLC\_MAC}}
\index{GSMTAP\_TYPE\_UMTS\_RLC\_MAC@{GSMTAP\_TYPE\_UMTS\_RLC\_MAC}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_TYPE\_UMTS\_RLC\_MAC}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+TYPE\+\_\+\+UMTS\+\_\+\+RLC\+\_\+\+MAC~0x0b}

\mbox{\label{gsmtap_8h_a3da9cb8f17807e6c810f739510506583}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_TYPE\_UMTS\_RRC@{GSMTAP\_TYPE\_UMTS\_RRC}}
\index{GSMTAP\_TYPE\_UMTS\_RRC@{GSMTAP\_TYPE\_UMTS\_RRC}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_TYPE\_UMTS\_RRC}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+TYPE\+\_\+\+UMTS\+\_\+\+RRC~0x0c}

\mbox{\label{gsmtap_8h_ad784d81f4dcd55a6bef72c6019f58b9a}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_TYPE\_WMX\_BURST@{GSMTAP\_TYPE\_WMX\_BURST}}
\index{GSMTAP\_TYPE\_WMX\_BURST@{GSMTAP\_TYPE\_WMX\_BURST}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_TYPE\_WMX\_BURST}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+TYPE\+\_\+\+WMX\+\_\+\+BURST~0x07    /$\ast$ Wi\+MAX burst $\ast$/}

\mbox{\label{gsmtap_8h_a8db05adec28e12ed9d5afc41592688e1}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_UDP\_PORT@{GSMTAP\_UDP\_PORT}}
\index{GSMTAP\_UDP\_PORT@{GSMTAP\_UDP\_PORT}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_UDP\_PORT}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+UDP\+\_\+\+PORT~4729}

\mbox{\label{gsmtap_8h_a9b21575ecd8ba89d4e09198dfffc1653}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_UMTS\_CH\_CCCH@{GSMTAP\_UMTS\_CH\_CCCH}}
\index{GSMTAP\_UMTS\_CH\_CCCH@{GSMTAP\_UMTS\_CH\_CCCH}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_UMTS\_CH\_CCCH}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+UMTS\+\_\+\+CH\+\_\+\+CCCH~0x02}

\mbox{\label{gsmtap_8h_af42a50acfce8079d1796629bde553362}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_UMTS\_CH\_DCCH@{GSMTAP\_UMTS\_CH\_DCCH}}
\index{GSMTAP\_UMTS\_CH\_DCCH@{GSMTAP\_UMTS\_CH\_DCCH}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_UMTS\_CH\_DCCH}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+UMTS\+\_\+\+CH\+\_\+\+DCCH~0x03}

\mbox{\label{gsmtap_8h_a146564d748122ae5b69df67b7ae7d89c}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_UMTS\_CH\_PCCH@{GSMTAP\_UMTS\_CH\_PCCH}}
\index{GSMTAP\_UMTS\_CH\_PCCH@{GSMTAP\_UMTS\_CH\_PCCH}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_UMTS\_CH\_PCCH}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+UMTS\+\_\+\+CH\+\_\+\+PCCH~0x01}

\mbox{\label{gsmtap_8h_a536563b1d85851e10c97d3901c8f3f85}} 
\index{gsmtap.h@{gsmtap.h}!GSMTAP\_VERSION@{GSMTAP\_VERSION}}
\index{GSMTAP\_VERSION@{GSMTAP\_VERSION}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{GSMTAP\_VERSION}
{\footnotesize\ttfamily \#define GSMTAP\+\_\+\+VERSION~0x02}



\doxysubsection{Enumeration Type Documentation}
\mbox{\label{gsmtap_8h_adf764cbdea00d65edcd07bb9953ad2b7}} 
\doxysubsubsection{anonymous enum}
{\footnotesize\ttfamily anonymous enum}

\begin{DoxyEnumFields}{Enumerator}
\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_RRC\_SUB\_DL\_DCCH\_Message@{GSMTAP\_RRC\_SUB\_DL\_DCCH\_Message}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_RRC\_SUB\_DL\_DCCH\_Message@{GSMTAP\_RRC\_SUB\_DL\_DCCH\_Message}}}\mbox{\label{gsmtap_8h_adf764cbdea00d65edcd07bb9953ad2b7ab031f4533874288ade7833ec76d05d3c}} 
GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+DL\+\_\+\+DCCH\+\_\+\+Message&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_RRC\_SUB\_UL\_DCCH\_Message@{GSMTAP\_RRC\_SUB\_UL\_DCCH\_Message}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_RRC\_SUB\_UL\_DCCH\_Message@{GSMTAP\_RRC\_SUB\_UL\_DCCH\_Message}}}\mbox{\label{gsmtap_8h_adf764cbdea00d65edcd07bb9953ad2b7a1a3a3718008510ccbd0927939e37afd7}} 
GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+UL\+\_\+\+DCCH\+\_\+\+Message&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_RRC\_SUB\_DL\_CCCH\_Message@{GSMTAP\_RRC\_SUB\_DL\_CCCH\_Message}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_RRC\_SUB\_DL\_CCCH\_Message@{GSMTAP\_RRC\_SUB\_DL\_CCCH\_Message}}}\mbox{\label{gsmtap_8h_adf764cbdea00d65edcd07bb9953ad2b7aa72d51500388e509b5182826afd30020}} 
GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+DL\+\_\+\+CCCH\+\_\+\+Message&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_RRC\_SUB\_UL\_CCCH\_Message@{GSMTAP\_RRC\_SUB\_UL\_CCCH\_Message}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_RRC\_SUB\_UL\_CCCH\_Message@{GSMTAP\_RRC\_SUB\_UL\_CCCH\_Message}}}\mbox{\label{gsmtap_8h_adf764cbdea00d65edcd07bb9953ad2b7a3093c92911bc0eba3ced487024345822}} 
GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+UL\+\_\+\+CCCH\+\_\+\+Message&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_RRC\_SUB\_PCCH\_Message@{GSMTAP\_RRC\_SUB\_PCCH\_Message}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_RRC\_SUB\_PCCH\_Message@{GSMTAP\_RRC\_SUB\_PCCH\_Message}}}\mbox{\label{gsmtap_8h_adf764cbdea00d65edcd07bb9953ad2b7a27a8c7c583981294368b1967fb87c48d}} 
GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+PCCH\+\_\+\+Message&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_RRC\_SUB\_DL\_SHCCH\_Message@{GSMTAP\_RRC\_SUB\_DL\_SHCCH\_Message}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_RRC\_SUB\_DL\_SHCCH\_Message@{GSMTAP\_RRC\_SUB\_DL\_SHCCH\_Message}}}\mbox{\label{gsmtap_8h_adf764cbdea00d65edcd07bb9953ad2b7a4f2b39589fc3fdd56741523b283f5680}} 
GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+DL\+\_\+\+SHCCH\+\_\+\+Message&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_RRC\_SUB\_UL\_SHCCH\_Message@{GSMTAP\_RRC\_SUB\_UL\_SHCCH\_Message}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_RRC\_SUB\_UL\_SHCCH\_Message@{GSMTAP\_RRC\_SUB\_UL\_SHCCH\_Message}}}\mbox{\label{gsmtap_8h_adf764cbdea00d65edcd07bb9953ad2b7af6945b17403a39aa3236e2e8f271afdc}} 
GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+UL\+\_\+\+SHCCH\+\_\+\+Message&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_RRC\_SUB\_BCCH\_FACH\_Message@{GSMTAP\_RRC\_SUB\_BCCH\_FACH\_Message}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_RRC\_SUB\_BCCH\_FACH\_Message@{GSMTAP\_RRC\_SUB\_BCCH\_FACH\_Message}}}\mbox{\label{gsmtap_8h_adf764cbdea00d65edcd07bb9953ad2b7ae112401440039d1b8897d85ccbbd2beb}} 
GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+BCCH\+\_\+\+FACH\+\_\+\+Message&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_RRC\_SUB\_BCCH\_BCH\_Message@{GSMTAP\_RRC\_SUB\_BCCH\_BCH\_Message}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_RRC\_SUB\_BCCH\_BCH\_Message@{GSMTAP\_RRC\_SUB\_BCCH\_BCH\_Message}}}\mbox{\label{gsmtap_8h_adf764cbdea00d65edcd07bb9953ad2b7a407c37cc7abceb71305a367d006b8572}} 
GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+BCCH\+\_\+\+BCH\+\_\+\+Message&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_RRC\_SUB\_MCCH\_Message@{GSMTAP\_RRC\_SUB\_MCCH\_Message}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_RRC\_SUB\_MCCH\_Message@{GSMTAP\_RRC\_SUB\_MCCH\_Message}}}\mbox{\label{gsmtap_8h_adf764cbdea00d65edcd07bb9953ad2b7a632ea204298221cfacfa48000948ae27}} 
GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+MCCH\+\_\+\+Message&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_RRC\_SUB\_MSCH\_Message@{GSMTAP\_RRC\_SUB\_MSCH\_Message}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_RRC\_SUB\_MSCH\_Message@{GSMTAP\_RRC\_SUB\_MSCH\_Message}}}\mbox{\label{gsmtap_8h_adf764cbdea00d65edcd07bb9953ad2b7af7e333caa28c34d4059c06c592e5e667}} 
GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+MSCH\+\_\+\+Message&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_RRC\_SUB\_HandoverToUTRANCommand@{GSMTAP\_RRC\_SUB\_HandoverToUTRANCommand}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_RRC\_SUB\_HandoverToUTRANCommand@{GSMTAP\_RRC\_SUB\_HandoverToUTRANCommand}}}\mbox{\label{gsmtap_8h_adf764cbdea00d65edcd07bb9953ad2b7ad5125d549a93d929d6c17f106499f41c}} 
GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Handover\+To\+UTRANCommand&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_RRC\_SUB\_InterRATHandoverInfo@{GSMTAP\_RRC\_SUB\_InterRATHandoverInfo}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_RRC\_SUB\_InterRATHandoverInfo@{GSMTAP\_RRC\_SUB\_InterRATHandoverInfo}}}\mbox{\label{gsmtap_8h_adf764cbdea00d65edcd07bb9953ad2b7a23c90e9339264c347e73e1896a3a8d22}} 
GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Inter\+RATHandover\+Info&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_RRC\_SUB\_SystemInformation\_BCH@{GSMTAP\_RRC\_SUB\_SystemInformation\_BCH}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_RRC\_SUB\_SystemInformation\_BCH@{GSMTAP\_RRC\_SUB\_SystemInformation\_BCH}}}\mbox{\label{gsmtap_8h_adf764cbdea00d65edcd07bb9953ad2b7a26ac98a5ef182d8994cce14c9bebd0f3}} 
GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+System\+Information\+\_\+\+BCH&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_RRC\_SUB\_System\_Information\_Container@{GSMTAP\_RRC\_SUB\_System\_Information\_Container}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_RRC\_SUB\_System\_Information\_Container@{GSMTAP\_RRC\_SUB\_System\_Information\_Container}}}\mbox{\label{gsmtap_8h_adf764cbdea00d65edcd07bb9953ad2b7a07c12214ef89d741779a60430c35edfa}} 
GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+System\+\_\+\+Information\+\_\+\+Container&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_RRC\_SUB\_UE\_RadioAccessCapabilityInfo@{GSMTAP\_RRC\_SUB\_UE\_RadioAccessCapabilityInfo}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_RRC\_SUB\_UE\_RadioAccessCapabilityInfo@{GSMTAP\_RRC\_SUB\_UE\_RadioAccessCapabilityInfo}}}\mbox{\label{gsmtap_8h_adf764cbdea00d65edcd07bb9953ad2b7a7f62230330d50b1476f5710d356bb520}} 
GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+UE\+\_\+\+Radio\+Access\+Capability\+Info&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_RRC\_SUB\_MasterInformationBlock@{GSMTAP\_RRC\_SUB\_MasterInformationBlock}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_RRC\_SUB\_MasterInformationBlock@{GSMTAP\_RRC\_SUB\_MasterInformationBlock}}}\mbox{\label{gsmtap_8h_adf764cbdea00d65edcd07bb9953ad2b7a1e2996f829e5a42623e7d4ab4c1259a2}} 
GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Master\+Information\+Block&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_RRC\_SUB\_SysInfoType1@{GSMTAP\_RRC\_SUB\_SysInfoType1}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_RRC\_SUB\_SysInfoType1@{GSMTAP\_RRC\_SUB\_SysInfoType1}}}\mbox{\label{gsmtap_8h_adf764cbdea00d65edcd07bb9953ad2b7a9561b31a5ce4a4510a3a7f44851e9799}} 
GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type1&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_RRC\_SUB\_SysInfoType2@{GSMTAP\_RRC\_SUB\_SysInfoType2}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_RRC\_SUB\_SysInfoType2@{GSMTAP\_RRC\_SUB\_SysInfoType2}}}\mbox{\label{gsmtap_8h_adf764cbdea00d65edcd07bb9953ad2b7a34c2720f1a0bd1f26c61ce4ff22976bb}} 
GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type2&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_RRC\_SUB\_SysInfoType3@{GSMTAP\_RRC\_SUB\_SysInfoType3}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_RRC\_SUB\_SysInfoType3@{GSMTAP\_RRC\_SUB\_SysInfoType3}}}\mbox{\label{gsmtap_8h_adf764cbdea00d65edcd07bb9953ad2b7a1a2b896b436dc36f8006503b2815dcc0}} 
GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type3&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_RRC\_SUB\_SysInfoType4@{GSMTAP\_RRC\_SUB\_SysInfoType4}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_RRC\_SUB\_SysInfoType4@{GSMTAP\_RRC\_SUB\_SysInfoType4}}}\mbox{\label{gsmtap_8h_adf764cbdea00d65edcd07bb9953ad2b7a16b23fd93a0021439d09ea5c86c02914}} 
GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type4&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_RRC\_SUB\_SysInfoType5@{GSMTAP\_RRC\_SUB\_SysInfoType5}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_RRC\_SUB\_SysInfoType5@{GSMTAP\_RRC\_SUB\_SysInfoType5}}}\mbox{\label{gsmtap_8h_adf764cbdea00d65edcd07bb9953ad2b7a5265e6843364a3c6545c5f87a829a0f4}} 
GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type5&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_RRC\_SUB\_SysInfoType5bis@{GSMTAP\_RRC\_SUB\_SysInfoType5bis}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_RRC\_SUB\_SysInfoType5bis@{GSMTAP\_RRC\_SUB\_SysInfoType5bis}}}\mbox{\label{gsmtap_8h_adf764cbdea00d65edcd07bb9953ad2b7a375471c228da838f8b8b91a6bd913d04}} 
GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type5bis&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_RRC\_SUB\_SysInfoType6@{GSMTAP\_RRC\_SUB\_SysInfoType6}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_RRC\_SUB\_SysInfoType6@{GSMTAP\_RRC\_SUB\_SysInfoType6}}}\mbox{\label{gsmtap_8h_adf764cbdea00d65edcd07bb9953ad2b7ad89f84dc511566eaf71dd6cceaca6a99}} 
GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type6&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_RRC\_SUB\_SysInfoType7@{GSMTAP\_RRC\_SUB\_SysInfoType7}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_RRC\_SUB\_SysInfoType7@{GSMTAP\_RRC\_SUB\_SysInfoType7}}}\mbox{\label{gsmtap_8h_adf764cbdea00d65edcd07bb9953ad2b7a542201850adf8cbfc50a4604cb76a048}} 
GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type7&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_RRC\_SUB\_SysInfoType8@{GSMTAP\_RRC\_SUB\_SysInfoType8}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_RRC\_SUB\_SysInfoType8@{GSMTAP\_RRC\_SUB\_SysInfoType8}}}\mbox{\label{gsmtap_8h_adf764cbdea00d65edcd07bb9953ad2b7afefea5630da298084fe587d66467eb1b}} 
GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type8&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_RRC\_SUB\_SysInfoType9@{GSMTAP\_RRC\_SUB\_SysInfoType9}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_RRC\_SUB\_SysInfoType9@{GSMTAP\_RRC\_SUB\_SysInfoType9}}}\mbox{\label{gsmtap_8h_adf764cbdea00d65edcd07bb9953ad2b7ae00c65aa4c39786090b12f675dea2786}} 
GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type9&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_RRC\_SUB\_SysInfoType10@{GSMTAP\_RRC\_SUB\_SysInfoType10}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_RRC\_SUB\_SysInfoType10@{GSMTAP\_RRC\_SUB\_SysInfoType10}}}\mbox{\label{gsmtap_8h_adf764cbdea00d65edcd07bb9953ad2b7a82db1eed4d14e81f006f4a5fae247598}} 
GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type10&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_RRC\_SUB\_SysInfoType11@{GSMTAP\_RRC\_SUB\_SysInfoType11}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_RRC\_SUB\_SysInfoType11@{GSMTAP\_RRC\_SUB\_SysInfoType11}}}\mbox{\label{gsmtap_8h_adf764cbdea00d65edcd07bb9953ad2b7a17fa1ab4ea3f93162f859e640767e773}} 
GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type11&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_RRC\_SUB\_SysInfoType11bis@{GSMTAP\_RRC\_SUB\_SysInfoType11bis}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_RRC\_SUB\_SysInfoType11bis@{GSMTAP\_RRC\_SUB\_SysInfoType11bis}}}\mbox{\label{gsmtap_8h_adf764cbdea00d65edcd07bb9953ad2b7a162f7d39a63b7287715d2290827c8014}} 
GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type11bis&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_RRC\_SUB\_SysInfoType12@{GSMTAP\_RRC\_SUB\_SysInfoType12}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_RRC\_SUB\_SysInfoType12@{GSMTAP\_RRC\_SUB\_SysInfoType12}}}\mbox{\label{gsmtap_8h_adf764cbdea00d65edcd07bb9953ad2b7acc09b86b543fdba7d6f0078536aaaca2}} 
GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type12&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_RRC\_SUB\_SysInfoType13@{GSMTAP\_RRC\_SUB\_SysInfoType13}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_RRC\_SUB\_SysInfoType13@{GSMTAP\_RRC\_SUB\_SysInfoType13}}}\mbox{\label{gsmtap_8h_adf764cbdea00d65edcd07bb9953ad2b7a4e4606f0b569853499b5c9656f406845}} 
GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type13&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_RRC\_SUB\_SysInfoType13\_1@{GSMTAP\_RRC\_SUB\_SysInfoType13\_1}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_RRC\_SUB\_SysInfoType13\_1@{GSMTAP\_RRC\_SUB\_SysInfoType13\_1}}}\mbox{\label{gsmtap_8h_adf764cbdea00d65edcd07bb9953ad2b7af1f581c229bbb0ce96ca2c0f0bf71a46}} 
GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type13\+\_\+1&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_RRC\_SUB\_SysInfoType13\_2@{GSMTAP\_RRC\_SUB\_SysInfoType13\_2}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_RRC\_SUB\_SysInfoType13\_2@{GSMTAP\_RRC\_SUB\_SysInfoType13\_2}}}\mbox{\label{gsmtap_8h_adf764cbdea00d65edcd07bb9953ad2b7a070b5ad741fd20dc3cc490ce0db4e615}} 
GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type13\+\_\+2&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_RRC\_SUB\_SysInfoType13\_3@{GSMTAP\_RRC\_SUB\_SysInfoType13\_3}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_RRC\_SUB\_SysInfoType13\_3@{GSMTAP\_RRC\_SUB\_SysInfoType13\_3}}}\mbox{\label{gsmtap_8h_adf764cbdea00d65edcd07bb9953ad2b7a5c405f061fbe111ac09502ed1052d2b5}} 
GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type13\+\_\+3&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_RRC\_SUB\_SysInfoType13\_4@{GSMTAP\_RRC\_SUB\_SysInfoType13\_4}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_RRC\_SUB\_SysInfoType13\_4@{GSMTAP\_RRC\_SUB\_SysInfoType13\_4}}}\mbox{\label{gsmtap_8h_adf764cbdea00d65edcd07bb9953ad2b7a84db3dbabd102621fca340746166d64f}} 
GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type13\+\_\+4&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_RRC\_SUB\_SysInfoType14@{GSMTAP\_RRC\_SUB\_SysInfoType14}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_RRC\_SUB\_SysInfoType14@{GSMTAP\_RRC\_SUB\_SysInfoType14}}}\mbox{\label{gsmtap_8h_adf764cbdea00d65edcd07bb9953ad2b7a28abf7ecb203b8764eb3982df3dc0d83}} 
GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type14&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_RRC\_SUB\_SysInfoType15@{GSMTAP\_RRC\_SUB\_SysInfoType15}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_RRC\_SUB\_SysInfoType15@{GSMTAP\_RRC\_SUB\_SysInfoType15}}}\mbox{\label{gsmtap_8h_adf764cbdea00d65edcd07bb9953ad2b7ad64947dcd939fc770c6968297b9a0112}} 
GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type15&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_RRC\_SUB\_SysInfoType15bis@{GSMTAP\_RRC\_SUB\_SysInfoType15bis}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_RRC\_SUB\_SysInfoType15bis@{GSMTAP\_RRC\_SUB\_SysInfoType15bis}}}\mbox{\label{gsmtap_8h_adf764cbdea00d65edcd07bb9953ad2b7a582e26c8bee326d5be30eab663acfaf3}} 
GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type15bis&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_RRC\_SUB\_SysInfoType15\_1@{GSMTAP\_RRC\_SUB\_SysInfoType15\_1}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_RRC\_SUB\_SysInfoType15\_1@{GSMTAP\_RRC\_SUB\_SysInfoType15\_1}}}\mbox{\label{gsmtap_8h_adf764cbdea00d65edcd07bb9953ad2b7ac481c2a700c33a3351907a2a2ef39c8a}} 
GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type15\+\_\+1&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_RRC\_SUB\_SysInfoType15\_1bis@{GSMTAP\_RRC\_SUB\_SysInfoType15\_1bis}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_RRC\_SUB\_SysInfoType15\_1bis@{GSMTAP\_RRC\_SUB\_SysInfoType15\_1bis}}}\mbox{\label{gsmtap_8h_adf764cbdea00d65edcd07bb9953ad2b7a5d3a2b6147d03a116634e09e72152769}} 
GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type15\+\_\+1bis&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_RRC\_SUB\_SysInfoType15\_2@{GSMTAP\_RRC\_SUB\_SysInfoType15\_2}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_RRC\_SUB\_SysInfoType15\_2@{GSMTAP\_RRC\_SUB\_SysInfoType15\_2}}}\mbox{\label{gsmtap_8h_adf764cbdea00d65edcd07bb9953ad2b7a365bcc94aef0e8332a665ddbfa66b922}} 
GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type15\+\_\+2&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_RRC\_SUB\_SysInfoType15\_2bis@{GSMTAP\_RRC\_SUB\_SysInfoType15\_2bis}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_RRC\_SUB\_SysInfoType15\_2bis@{GSMTAP\_RRC\_SUB\_SysInfoType15\_2bis}}}\mbox{\label{gsmtap_8h_adf764cbdea00d65edcd07bb9953ad2b7a60c0b15bd4eab794c63cf998e3a51510}} 
GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type15\+\_\+2bis&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_RRC\_SUB\_SysInfoType15\_2ter@{GSMTAP\_RRC\_SUB\_SysInfoType15\_2ter}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_RRC\_SUB\_SysInfoType15\_2ter@{GSMTAP\_RRC\_SUB\_SysInfoType15\_2ter}}}\mbox{\label{gsmtap_8h_adf764cbdea00d65edcd07bb9953ad2b7a6e257db9ad9d55fc8668622b7eb23010}} 
GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type15\+\_\+2ter&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_RRC\_SUB\_SysInfoType15\_3@{GSMTAP\_RRC\_SUB\_SysInfoType15\_3}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_RRC\_SUB\_SysInfoType15\_3@{GSMTAP\_RRC\_SUB\_SysInfoType15\_3}}}\mbox{\label{gsmtap_8h_adf764cbdea00d65edcd07bb9953ad2b7ab3cb4d69344df931eadc4ad0973995bc}} 
GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type15\+\_\+3&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_RRC\_SUB\_SysInfoType15\_3bis@{GSMTAP\_RRC\_SUB\_SysInfoType15\_3bis}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_RRC\_SUB\_SysInfoType15\_3bis@{GSMTAP\_RRC\_SUB\_SysInfoType15\_3bis}}}\mbox{\label{gsmtap_8h_adf764cbdea00d65edcd07bb9953ad2b7ada5e20914afaf87a787dea3cda6e0106}} 
GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type15\+\_\+3bis&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_RRC\_SUB\_SysInfoType15\_4@{GSMTAP\_RRC\_SUB\_SysInfoType15\_4}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_RRC\_SUB\_SysInfoType15\_4@{GSMTAP\_RRC\_SUB\_SysInfoType15\_4}}}\mbox{\label{gsmtap_8h_adf764cbdea00d65edcd07bb9953ad2b7a4e9b0954530afcf69d22c8195b7767e1}} 
GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type15\+\_\+4&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_RRC\_SUB\_SysInfoType15\_5@{GSMTAP\_RRC\_SUB\_SysInfoType15\_5}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_RRC\_SUB\_SysInfoType15\_5@{GSMTAP\_RRC\_SUB\_SysInfoType15\_5}}}\mbox{\label{gsmtap_8h_adf764cbdea00d65edcd07bb9953ad2b7ac90b05baa5f637d45af691fa797a9cab}} 
GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type15\+\_\+5&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_RRC\_SUB\_SysInfoType15\_6@{GSMTAP\_RRC\_SUB\_SysInfoType15\_6}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_RRC\_SUB\_SysInfoType15\_6@{GSMTAP\_RRC\_SUB\_SysInfoType15\_6}}}\mbox{\label{gsmtap_8h_adf764cbdea00d65edcd07bb9953ad2b7a388970527e5831dfcfc18603456994c7}} 
GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type15\+\_\+6&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_RRC\_SUB\_SysInfoType15\_7@{GSMTAP\_RRC\_SUB\_SysInfoType15\_7}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_RRC\_SUB\_SysInfoType15\_7@{GSMTAP\_RRC\_SUB\_SysInfoType15\_7}}}\mbox{\label{gsmtap_8h_adf764cbdea00d65edcd07bb9953ad2b7a17c3d0bde7d6a5944a46976d0302888e}} 
GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type15\+\_\+7&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_RRC\_SUB\_SysInfoType15\_8@{GSMTAP\_RRC\_SUB\_SysInfoType15\_8}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_RRC\_SUB\_SysInfoType15\_8@{GSMTAP\_RRC\_SUB\_SysInfoType15\_8}}}\mbox{\label{gsmtap_8h_adf764cbdea00d65edcd07bb9953ad2b7ad9d8830462c3123c07e8761cfc9495a5}} 
GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type15\+\_\+8&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_RRC\_SUB\_SysInfoType16@{GSMTAP\_RRC\_SUB\_SysInfoType16}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_RRC\_SUB\_SysInfoType16@{GSMTAP\_RRC\_SUB\_SysInfoType16}}}\mbox{\label{gsmtap_8h_adf764cbdea00d65edcd07bb9953ad2b7a1b8f08e057bf1cd74709305c05d25ff9}} 
GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type16&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_RRC\_SUB\_SysInfoType17@{GSMTAP\_RRC\_SUB\_SysInfoType17}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_RRC\_SUB\_SysInfoType17@{GSMTAP\_RRC\_SUB\_SysInfoType17}}}\mbox{\label{gsmtap_8h_adf764cbdea00d65edcd07bb9953ad2b7a954c175d2c0fb80da5958dd3ae5414b5}} 
GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type17&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_RRC\_SUB\_SysInfoType18@{GSMTAP\_RRC\_SUB\_SysInfoType18}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_RRC\_SUB\_SysInfoType18@{GSMTAP\_RRC\_SUB\_SysInfoType18}}}\mbox{\label{gsmtap_8h_adf764cbdea00d65edcd07bb9953ad2b7a06bf2234faa27c331d533f6a3f4c6b23}} 
GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type18&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_RRC\_SUB\_SysInfoType19@{GSMTAP\_RRC\_SUB\_SysInfoType19}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_RRC\_SUB\_SysInfoType19@{GSMTAP\_RRC\_SUB\_SysInfoType19}}}\mbox{\label{gsmtap_8h_adf764cbdea00d65edcd07bb9953ad2b7a90ea69ee109882fda0b26e7ea1cdbfa7}} 
GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type19&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_RRC\_SUB\_SysInfoType20@{GSMTAP\_RRC\_SUB\_SysInfoType20}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_RRC\_SUB\_SysInfoType20@{GSMTAP\_RRC\_SUB\_SysInfoType20}}}\mbox{\label{gsmtap_8h_adf764cbdea00d65edcd07bb9953ad2b7ad6885089c00e549d3da75b45eae72853}} 
GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type20&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_RRC\_SUB\_SysInfoType21@{GSMTAP\_RRC\_SUB\_SysInfoType21}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_RRC\_SUB\_SysInfoType21@{GSMTAP\_RRC\_SUB\_SysInfoType21}}}\mbox{\label{gsmtap_8h_adf764cbdea00d65edcd07bb9953ad2b7a0bc41bd8686cef0ed549f1ca5fbcf4ba}} 
GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type21&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_RRC\_SUB\_SysInfoType22@{GSMTAP\_RRC\_SUB\_SysInfoType22}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_RRC\_SUB\_SysInfoType22@{GSMTAP\_RRC\_SUB\_SysInfoType22}}}\mbox{\label{gsmtap_8h_adf764cbdea00d65edcd07bb9953ad2b7aac8b3a243e4cea60c130c535ea94c00a}} 
GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type22&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_RRC\_SUB\_SysInfoTypeSB1@{GSMTAP\_RRC\_SUB\_SysInfoTypeSB1}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_RRC\_SUB\_SysInfoTypeSB1@{GSMTAP\_RRC\_SUB\_SysInfoTypeSB1}}}\mbox{\label{gsmtap_8h_adf764cbdea00d65edcd07bb9953ad2b7a03c228e5aa8910c813664444467810f5}} 
GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type\+SB1&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_RRC\_SUB\_SysInfoTypeSB2@{GSMTAP\_RRC\_SUB\_SysInfoTypeSB2}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_RRC\_SUB\_SysInfoTypeSB2@{GSMTAP\_RRC\_SUB\_SysInfoTypeSB2}}}\mbox{\label{gsmtap_8h_adf764cbdea00d65edcd07bb9953ad2b7adaa6d15867a4c90a4966cb3b2555e160}} 
GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Sys\+Info\+Type\+SB2&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_RRC\_SUB\_ToTargetRNC\_Container@{GSMTAP\_RRC\_SUB\_ToTargetRNC\_Container}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_RRC\_SUB\_ToTargetRNC\_Container@{GSMTAP\_RRC\_SUB\_ToTargetRNC\_Container}}}\mbox{\label{gsmtap_8h_adf764cbdea00d65edcd07bb9953ad2b7a96c27b1d442f853d6b06470b4a90fc36}} 
GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+To\+Target\+RNC\+\_\+\+Container&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_RRC\_SUB\_TargetRNC\_ToSourceRNC\_Container@{GSMTAP\_RRC\_SUB\_TargetRNC\_ToSourceRNC\_Container}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_RRC\_SUB\_TargetRNC\_ToSourceRNC\_Container@{GSMTAP\_RRC\_SUB\_TargetRNC\_ToSourceRNC\_Container}}}\mbox{\label{gsmtap_8h_adf764cbdea00d65edcd07bb9953ad2b7a4da839f5f38ac2b96af61d29511e0c66}} 
GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+Target\+RNC\+\_\+\+To\+Source\+RNC\+\_\+\+Container&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_RRC\_SUB\_MAX@{GSMTAP\_RRC\_SUB\_MAX}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_RRC\_SUB\_MAX@{GSMTAP\_RRC\_SUB\_MAX}}}\mbox{\label{gsmtap_8h_adf764cbdea00d65edcd07bb9953ad2b7a2b277cde351bcd2d13c44818cf1e4924}} 
GSMTAP\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+MAX&\\
\hline

\end{DoxyEnumFields}
\mbox{\label{gsmtap_8h_a99fb83031ce9923c84392b4e92f956b5}} 
\doxysubsubsection{anonymous enum}
{\footnotesize\ttfamily anonymous enum}

\begin{DoxyEnumFields}{Enumerator}
\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_LTE\_RRC\_SUB\_DL\_CCCH\_Message@{GSMTAP\_LTE\_RRC\_SUB\_DL\_CCCH\_Message}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_LTE\_RRC\_SUB\_DL\_CCCH\_Message@{GSMTAP\_LTE\_RRC\_SUB\_DL\_CCCH\_Message}}}\mbox{\label{gsmtap_8h_a99fb83031ce9923c84392b4e92f956b5a28510b8b4baea4a2b31bc6f424d4c99c}} 
GSMTAP\+\_\+\+LTE\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+DL\+\_\+\+CCCH\+\_\+\+Message&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_LTE\_RRC\_SUB\_DL\_DCCH\_Message@{GSMTAP\_LTE\_RRC\_SUB\_DL\_DCCH\_Message}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_LTE\_RRC\_SUB\_DL\_DCCH\_Message@{GSMTAP\_LTE\_RRC\_SUB\_DL\_DCCH\_Message}}}\mbox{\label{gsmtap_8h_a99fb83031ce9923c84392b4e92f956b5a50f1189b365aa0c175357e3d2e975b03}} 
GSMTAP\+\_\+\+LTE\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+DL\+\_\+\+DCCH\+\_\+\+Message&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_LTE\_RRC\_SUB\_UL\_CCCH\_Message@{GSMTAP\_LTE\_RRC\_SUB\_UL\_CCCH\_Message}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_LTE\_RRC\_SUB\_UL\_CCCH\_Message@{GSMTAP\_LTE\_RRC\_SUB\_UL\_CCCH\_Message}}}\mbox{\label{gsmtap_8h_a99fb83031ce9923c84392b4e92f956b5a6425c21c79effd4b05a17ee1427d2ba3}} 
GSMTAP\+\_\+\+LTE\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+UL\+\_\+\+CCCH\+\_\+\+Message&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_LTE\_RRC\_SUB\_UL\_DCCH\_Message@{GSMTAP\_LTE\_RRC\_SUB\_UL\_DCCH\_Message}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_LTE\_RRC\_SUB\_UL\_DCCH\_Message@{GSMTAP\_LTE\_RRC\_SUB\_UL\_DCCH\_Message}}}\mbox{\label{gsmtap_8h_a99fb83031ce9923c84392b4e92f956b5a89503a5454bce0029a0337f87a8235b0}} 
GSMTAP\+\_\+\+LTE\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+UL\+\_\+\+DCCH\+\_\+\+Message&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_LTE\_RRC\_SUB\_BCCH\_BCH\_Message@{GSMTAP\_LTE\_RRC\_SUB\_BCCH\_BCH\_Message}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_LTE\_RRC\_SUB\_BCCH\_BCH\_Message@{GSMTAP\_LTE\_RRC\_SUB\_BCCH\_BCH\_Message}}}\mbox{\label{gsmtap_8h_a99fb83031ce9923c84392b4e92f956b5af99e61ecb0aa6998f6cf088db6ee0dfc}} 
GSMTAP\+\_\+\+LTE\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+BCCH\+\_\+\+BCH\+\_\+\+Message&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_LTE\_RRC\_SUB\_BCCH\_DL\_SCH\_Message@{GSMTAP\_LTE\_RRC\_SUB\_BCCH\_DL\_SCH\_Message}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_LTE\_RRC\_SUB\_BCCH\_DL\_SCH\_Message@{GSMTAP\_LTE\_RRC\_SUB\_BCCH\_DL\_SCH\_Message}}}\mbox{\label{gsmtap_8h_a99fb83031ce9923c84392b4e92f956b5a7612b8a0ad7a94058ffeb70363c0133a}} 
GSMTAP\+\_\+\+LTE\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+BCCH\+\_\+\+DL\+\_\+\+SCH\+\_\+\+Message&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_LTE\_RRC\_SUB\_PCCH\_Message@{GSMTAP\_LTE\_RRC\_SUB\_PCCH\_Message}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_LTE\_RRC\_SUB\_PCCH\_Message@{GSMTAP\_LTE\_RRC\_SUB\_PCCH\_Message}}}\mbox{\label{gsmtap_8h_a99fb83031ce9923c84392b4e92f956b5a91cbf61cde02b56c320fb71102c0ab55}} 
GSMTAP\+\_\+\+LTE\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+PCCH\+\_\+\+Message&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_LTE\_RRC\_SUB\_MCCH\_Message@{GSMTAP\_LTE\_RRC\_SUB\_MCCH\_Message}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_LTE\_RRC\_SUB\_MCCH\_Message@{GSMTAP\_LTE\_RRC\_SUB\_MCCH\_Message}}}\mbox{\label{gsmtap_8h_a99fb83031ce9923c84392b4e92f956b5a09d83be3b069681c4ba15c1ab87c7804}} 
GSMTAP\+\_\+\+LTE\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+MCCH\+\_\+\+Message&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_LTE\_RRC\_SUB\_BCCH\_BCH\_Message\_MBMS@{GSMTAP\_LTE\_RRC\_SUB\_BCCH\_BCH\_Message\_MBMS}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_LTE\_RRC\_SUB\_BCCH\_BCH\_Message\_MBMS@{GSMTAP\_LTE\_RRC\_SUB\_BCCH\_BCH\_Message\_MBMS}}}\mbox{\label{gsmtap_8h_a99fb83031ce9923c84392b4e92f956b5a55b1c955f97f78042cfac54eff616de0}} 
GSMTAP\+\_\+\+LTE\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+BCCH\+\_\+\+BCH\+\_\+\+Message\+\_\+\+MBMS&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_LTE\_RRC\_SUB\_BCCH\_DL\_SCH\_Message\_BR@{GSMTAP\_LTE\_RRC\_SUB\_BCCH\_DL\_SCH\_Message\_BR}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_LTE\_RRC\_SUB\_BCCH\_DL\_SCH\_Message\_BR@{GSMTAP\_LTE\_RRC\_SUB\_BCCH\_DL\_SCH\_Message\_BR}}}\mbox{\label{gsmtap_8h_a99fb83031ce9923c84392b4e92f956b5a1a20d97f86dd2d9f982544d80c5c8b02}} 
GSMTAP\+\_\+\+LTE\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+BCCH\+\_\+\+DL\+\_\+\+SCH\+\_\+\+Message\+\_\+\+BR&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_LTE\_RRC\_SUB\_BCCH\_DL\_SCH\_Message\_MBMS@{GSMTAP\_LTE\_RRC\_SUB\_BCCH\_DL\_SCH\_Message\_MBMS}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_LTE\_RRC\_SUB\_BCCH\_DL\_SCH\_Message\_MBMS@{GSMTAP\_LTE\_RRC\_SUB\_BCCH\_DL\_SCH\_Message\_MBMS}}}\mbox{\label{gsmtap_8h_a99fb83031ce9923c84392b4e92f956b5a6cc396ca66b4ea22c33daff9a9cf4b63}} 
GSMTAP\+\_\+\+LTE\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+BCCH\+\_\+\+DL\+\_\+\+SCH\+\_\+\+Message\+\_\+\+MBMS&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_LTE\_RRC\_SUB\_SC\_MCCH\_Message@{GSMTAP\_LTE\_RRC\_SUB\_SC\_MCCH\_Message}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_LTE\_RRC\_SUB\_SC\_MCCH\_Message@{GSMTAP\_LTE\_RRC\_SUB\_SC\_MCCH\_Message}}}\mbox{\label{gsmtap_8h_a99fb83031ce9923c84392b4e92f956b5a633d77f137481dd6d1bc3756d4f2bd6b}} 
GSMTAP\+\_\+\+LTE\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+SC\+\_\+\+MCCH\+\_\+\+Message&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_LTE\_RRC\_SUB\_SBCCH\_SL\_BCH\_Message@{GSMTAP\_LTE\_RRC\_SUB\_SBCCH\_SL\_BCH\_Message}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_LTE\_RRC\_SUB\_SBCCH\_SL\_BCH\_Message@{GSMTAP\_LTE\_RRC\_SUB\_SBCCH\_SL\_BCH\_Message}}}\mbox{\label{gsmtap_8h_a99fb83031ce9923c84392b4e92f956b5a44b8f711993cc8f224c88f23f2b49f4f}} 
GSMTAP\+\_\+\+LTE\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+SBCCH\+\_\+\+SL\+\_\+\+BCH\+\_\+\+Message&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_LTE\_RRC\_SUB\_SBCCH\_SL\_BCH\_Message\_V2X@{GSMTAP\_LTE\_RRC\_SUB\_SBCCH\_SL\_BCH\_Message\_V2X}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_LTE\_RRC\_SUB\_SBCCH\_SL\_BCH\_Message\_V2X@{GSMTAP\_LTE\_RRC\_SUB\_SBCCH\_SL\_BCH\_Message\_V2X}}}\mbox{\label{gsmtap_8h_a99fb83031ce9923c84392b4e92f956b5a539046ccc1c7077e43b04bdf99e45823}} 
GSMTAP\+\_\+\+LTE\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+SBCCH\+\_\+\+SL\+\_\+\+BCH\+\_\+\+Message\+\_\+\+V2X&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_LTE\_RRC\_SUB\_DL\_CCCH\_Message\_NB@{GSMTAP\_LTE\_RRC\_SUB\_DL\_CCCH\_Message\_NB}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_LTE\_RRC\_SUB\_DL\_CCCH\_Message\_NB@{GSMTAP\_LTE\_RRC\_SUB\_DL\_CCCH\_Message\_NB}}}\mbox{\label{gsmtap_8h_a99fb83031ce9923c84392b4e92f956b5a2e4872e6fa30df9b40e634bb68fe035e}} 
GSMTAP\+\_\+\+LTE\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+DL\+\_\+\+CCCH\+\_\+\+Message\+\_\+\+NB&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_LTE\_RRC\_SUB\_DL\_DCCH\_Message\_NB@{GSMTAP\_LTE\_RRC\_SUB\_DL\_DCCH\_Message\_NB}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_LTE\_RRC\_SUB\_DL\_DCCH\_Message\_NB@{GSMTAP\_LTE\_RRC\_SUB\_DL\_DCCH\_Message\_NB}}}\mbox{\label{gsmtap_8h_a99fb83031ce9923c84392b4e92f956b5aab543603e8139ec21df5b5f8f92393e5}} 
GSMTAP\+\_\+\+LTE\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+DL\+\_\+\+DCCH\+\_\+\+Message\+\_\+\+NB&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_LTE\_RRC\_SUB\_UL\_CCCH\_Message\_NB@{GSMTAP\_LTE\_RRC\_SUB\_UL\_CCCH\_Message\_NB}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_LTE\_RRC\_SUB\_UL\_CCCH\_Message\_NB@{GSMTAP\_LTE\_RRC\_SUB\_UL\_CCCH\_Message\_NB}}}\mbox{\label{gsmtap_8h_a99fb83031ce9923c84392b4e92f956b5a566ce53b8507c58c47c522f6277f9250}} 
GSMTAP\+\_\+\+LTE\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+UL\+\_\+\+CCCH\+\_\+\+Message\+\_\+\+NB&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_LTE\_RRC\_SUB\_UL\_DCCH\_Message\_NB@{GSMTAP\_LTE\_RRC\_SUB\_UL\_DCCH\_Message\_NB}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_LTE\_RRC\_SUB\_UL\_DCCH\_Message\_NB@{GSMTAP\_LTE\_RRC\_SUB\_UL\_DCCH\_Message\_NB}}}\mbox{\label{gsmtap_8h_a99fb83031ce9923c84392b4e92f956b5a803ddfd33e4e8f52e58d6edc3bbd9e2d}} 
GSMTAP\+\_\+\+LTE\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+UL\+\_\+\+DCCH\+\_\+\+Message\+\_\+\+NB&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_LTE\_RRC\_SUB\_BCCH\_BCH\_Message\_NB@{GSMTAP\_LTE\_RRC\_SUB\_BCCH\_BCH\_Message\_NB}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_LTE\_RRC\_SUB\_BCCH\_BCH\_Message\_NB@{GSMTAP\_LTE\_RRC\_SUB\_BCCH\_BCH\_Message\_NB}}}\mbox{\label{gsmtap_8h_a99fb83031ce9923c84392b4e92f956b5ac8dde45791136bd8d4df6ecccde2f019}} 
GSMTAP\+\_\+\+LTE\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+BCCH\+\_\+\+BCH\+\_\+\+Message\+\_\+\+NB&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_LTE\_RRC\_SUB\_BCCH\_BCH\_Message\_TDD\_NB@{GSMTAP\_LTE\_RRC\_SUB\_BCCH\_BCH\_Message\_TDD\_NB}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_LTE\_RRC\_SUB\_BCCH\_BCH\_Message\_TDD\_NB@{GSMTAP\_LTE\_RRC\_SUB\_BCCH\_BCH\_Message\_TDD\_NB}}}\mbox{\label{gsmtap_8h_a99fb83031ce9923c84392b4e92f956b5a0adccefde4114d606bf8f059923ad807}} 
GSMTAP\+\_\+\+LTE\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+BCCH\+\_\+\+BCH\+\_\+\+Message\+\_\+\+TDD\+\_\+\+NB&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_LTE\_RRC\_SUB\_BCCH\_DL\_SCH\_Message\_NB@{GSMTAP\_LTE\_RRC\_SUB\_BCCH\_DL\_SCH\_Message\_NB}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_LTE\_RRC\_SUB\_BCCH\_DL\_SCH\_Message\_NB@{GSMTAP\_LTE\_RRC\_SUB\_BCCH\_DL\_SCH\_Message\_NB}}}\mbox{\label{gsmtap_8h_a99fb83031ce9923c84392b4e92f956b5a47d4d7fe0908eb26b87996fc78b2c3ad}} 
GSMTAP\+\_\+\+LTE\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+BCCH\+\_\+\+DL\+\_\+\+SCH\+\_\+\+Message\+\_\+\+NB&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_LTE\_RRC\_SUB\_PCCH\_Message\_NB@{GSMTAP\_LTE\_RRC\_SUB\_PCCH\_Message\_NB}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_LTE\_RRC\_SUB\_PCCH\_Message\_NB@{GSMTAP\_LTE\_RRC\_SUB\_PCCH\_Message\_NB}}}\mbox{\label{gsmtap_8h_a99fb83031ce9923c84392b4e92f956b5ac1efb73b1050a8f124e461acc75bb852}} 
GSMTAP\+\_\+\+LTE\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+PCCH\+\_\+\+Message\+\_\+\+NB&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_LTE\_RRC\_SUB\_SC\_MCCH\_Message\_NB@{GSMTAP\_LTE\_RRC\_SUB\_SC\_MCCH\_Message\_NB}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_LTE\_RRC\_SUB\_SC\_MCCH\_Message\_NB@{GSMTAP\_LTE\_RRC\_SUB\_SC\_MCCH\_Message\_NB}}}\mbox{\label{gsmtap_8h_a99fb83031ce9923c84392b4e92f956b5af7aea0c6775e10323699e4a4153c8bcc}} 
GSMTAP\+\_\+\+LTE\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+SC\+\_\+\+MCCH\+\_\+\+Message\+\_\+\+NB&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_LTE\_RRC\_SUB\_MAX@{GSMTAP\_LTE\_RRC\_SUB\_MAX}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_LTE\_RRC\_SUB\_MAX@{GSMTAP\_LTE\_RRC\_SUB\_MAX}}}\mbox{\label{gsmtap_8h_a99fb83031ce9923c84392b4e92f956b5a54d403de52b7f16aa8c0c05ad58c39d8}} 
GSMTAP\+\_\+\+LTE\+\_\+\+RRC\+\_\+\+SUB\+\_\+\+MAX&\\
\hline

\end{DoxyEnumFields}
\mbox{\label{gsmtap_8h_abc6126af1d45847bc59afa0aa3216b04}} 
\doxysubsubsection{anonymous enum}
{\footnotesize\ttfamily anonymous enum}

\begin{DoxyEnumFields}{Enumerator}
\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_LTE\_NAS\_PLAIN@{GSMTAP\_LTE\_NAS\_PLAIN}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_LTE\_NAS\_PLAIN@{GSMTAP\_LTE\_NAS\_PLAIN}}}\mbox{\label{gsmtap_8h_abc6126af1d45847bc59afa0aa3216b04afbc8c5258a122a1f10617bdf301a9978}} 
GSMTAP\+\_\+\+LTE\+\_\+\+NAS\+\_\+\+PLAIN&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_LTE\_NAS\_SEC\_HEADER@{GSMTAP\_LTE\_NAS\_SEC\_HEADER}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_LTE\_NAS\_SEC\_HEADER@{GSMTAP\_LTE\_NAS\_SEC\_HEADER}}}\mbox{\label{gsmtap_8h_abc6126af1d45847bc59afa0aa3216b04a2e6c928fdc42eaf5774b9433f492bab8}} 
GSMTAP\+\_\+\+LTE\+\_\+\+NAS\+\_\+\+SEC\+\_\+\+HEADER&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_LTE\_NAS\_SUB\_MAX@{GSMTAP\_LTE\_NAS\_SUB\_MAX}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_LTE\_NAS\_SUB\_MAX@{GSMTAP\_LTE\_NAS\_SUB\_MAX}}}\mbox{\label{gsmtap_8h_abc6126af1d45847bc59afa0aa3216b04a1fc0e602744b50feb636701cb763f707}} 
GSMTAP\+\_\+\+LTE\+\_\+\+NAS\+\_\+\+SUB\+\_\+\+MAX&\\
\hline

\end{DoxyEnumFields}
\mbox{\label{gsmtap_8h_a32746df3f332bb431908704613166fe9}} 
\index{gsmtap.h@{gsmtap.h}!gsmtap\_um\_voice\_type@{gsmtap\_um\_voice\_type}}
\index{gsmtap\_um\_voice\_type@{gsmtap\_um\_voice\_type}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{gsmtap\_um\_voice\_type}
{\footnotesize\ttfamily enum \textbf{ gsmtap\+\_\+um\+\_\+voice\+\_\+type}}



First byte of type==GSMTAP\+\_\+\+TYPE\+\_\+\+UM sub\+\_\+type==GSMTAP\+\_\+\+CHANNEL\+\_\+\+VOICE payload. 

\begin{DoxyEnumFields}{Enumerator}
\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_UM\_VOICE\_HR@{GSMTAP\_UM\_VOICE\_HR}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_UM\_VOICE\_HR@{GSMTAP\_UM\_VOICE\_HR}}}\mbox{\label{gsmtap_8h_a32746df3f332bb431908704613166fe9ad617dee776a3d9b99d21634771c2c7c6}} 
GSMTAP\+\_\+\+UM\+\_\+\+VOICE\+\_\+\+HR&1 byte TOC + 112 bits (14 octets) = 15 octets payload; Reference is RFC5993 Section 5.\+2.\+1 + 3GPP TS 46.\+030 Annex B \\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_UM\_VOICE\_FR@{GSMTAP\_UM\_VOICE\_FR}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_UM\_VOICE\_FR@{GSMTAP\_UM\_VOICE\_FR}}}\mbox{\label{gsmtap_8h_a32746df3f332bb431908704613166fe9ae9d324e6164e36189811811d410fe8a8}} 
GSMTAP\+\_\+\+UM\+\_\+\+VOICE\+\_\+\+FR&33 payload bytes; Reference is RFC3551 Section 4.\+5.\+8.\+1 \\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_UM\_VOICE\_EFR@{GSMTAP\_UM\_VOICE\_EFR}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_UM\_VOICE\_EFR@{GSMTAP\_UM\_VOICE\_EFR}}}\mbox{\label{gsmtap_8h_a32746df3f332bb431908704613166fe9a72ecd9612136474e0015f429c094cbbc}} 
GSMTAP\+\_\+\+UM\+\_\+\+VOICE\+\_\+\+EFR&31 payload bytes; Reference is RFC3551 Section 4.\+5.\+9 + ETSI TS 101 318 \\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_UM\_VOICE\_AMR@{GSMTAP\_UM\_VOICE\_AMR}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_UM\_VOICE\_AMR@{GSMTAP\_UM\_VOICE\_AMR}}}\mbox{\label{gsmtap_8h_a32746df3f332bb431908704613166fe9a7645f5288bcd49021d21b84ddad390f9}} 
GSMTAP\+\_\+\+UM\+\_\+\+VOICE\+\_\+\+AMR&1 byte TOC + 5..31 bytes = 6..32 bytes payload; RFC4867 octet-\/aligned \\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_UM\_VOICE\_AMR\_SID\_BAD@{GSMTAP\_UM\_VOICE\_AMR\_SID\_BAD}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_UM\_VOICE\_AMR\_SID\_BAD@{GSMTAP\_UM\_VOICE\_AMR\_SID\_BAD}}}\mbox{\label{gsmtap_8h_a32746df3f332bb431908704613166fe9ad60d2ab32beb1e10d026cd142a63669b}} 
GSMTAP\+\_\+\+UM\+\_\+\+VOICE\+\_\+\+AMR\+\_\+\+SID\+\_\+\+BAD&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_UM\_VOICE\_AMR\_ONSET@{GSMTAP\_UM\_VOICE\_AMR\_ONSET}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_UM\_VOICE\_AMR\_ONSET@{GSMTAP\_UM\_VOICE\_AMR\_ONSET}}}\mbox{\label{gsmtap_8h_a32746df3f332bb431908704613166fe9a4ec17e9a197e9ceedcba78581e1b63de}} 
GSMTAP\+\_\+\+UM\+\_\+\+VOICE\+\_\+\+AMR\+\_\+\+ONSET&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_UM\_VOICE\_AMR\_RATSCCH@{GSMTAP\_UM\_VOICE\_AMR\_RATSCCH}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_UM\_VOICE\_AMR\_RATSCCH@{GSMTAP\_UM\_VOICE\_AMR\_RATSCCH}}}\mbox{\label{gsmtap_8h_a32746df3f332bb431908704613166fe9aa5159b8c1887fa1826f0aa7ec191d1eb}} 
GSMTAP\+\_\+\+UM\+\_\+\+VOICE\+\_\+\+AMR\+\_\+\+RATSCCH&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_UM\_VOICE\_AMR\_SID\_UPDATE\_INH@{GSMTAP\_UM\_VOICE\_AMR\_SID\_UPDATE\_INH}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_UM\_VOICE\_AMR\_SID\_UPDATE\_INH@{GSMTAP\_UM\_VOICE\_AMR\_SID\_UPDATE\_INH}}}\mbox{\label{gsmtap_8h_a32746df3f332bb431908704613166fe9a30db19b8f3065851b92024b2981e7026}} 
GSMTAP\+\_\+\+UM\+\_\+\+VOICE\+\_\+\+AMR\+\_\+\+SID\+\_\+\+UPDATE\+\_\+\+INH&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_UM\_VOICE\_AMR\_SID\_FIRST\_P1@{GSMTAP\_UM\_VOICE\_AMR\_SID\_FIRST\_P1}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_UM\_VOICE\_AMR\_SID\_FIRST\_P1@{GSMTAP\_UM\_VOICE\_AMR\_SID\_FIRST\_P1}}}\mbox{\label{gsmtap_8h_a32746df3f332bb431908704613166fe9ad0ce351c8a6eff774d3b9ec767288096}} 
GSMTAP\+\_\+\+UM\+\_\+\+VOICE\+\_\+\+AMR\+\_\+\+SID\+\_\+\+FIRST\+\_\+\+P1&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_UM\_VOICE\_AMR\_SID\_FIRST\_P2@{GSMTAP\_UM\_VOICE\_AMR\_SID\_FIRST\_P2}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_UM\_VOICE\_AMR\_SID\_FIRST\_P2@{GSMTAP\_UM\_VOICE\_AMR\_SID\_FIRST\_P2}}}\mbox{\label{gsmtap_8h_a32746df3f332bb431908704613166fe9ab5eec005456db3d1d4c76268fda5bdec}} 
GSMTAP\+\_\+\+UM\+\_\+\+VOICE\+\_\+\+AMR\+\_\+\+SID\+\_\+\+FIRST\+\_\+\+P2&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_UM\_VOICE\_AMR\_SID\_FIRST\_INH@{GSMTAP\_UM\_VOICE\_AMR\_SID\_FIRST\_INH}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_UM\_VOICE\_AMR\_SID\_FIRST\_INH@{GSMTAP\_UM\_VOICE\_AMR\_SID\_FIRST\_INH}}}\mbox{\label{gsmtap_8h_a32746df3f332bb431908704613166fe9a79a3574cab3ec92e5e889ca146ae11e8}} 
GSMTAP\+\_\+\+UM\+\_\+\+VOICE\+\_\+\+AMR\+\_\+\+SID\+\_\+\+FIRST\+\_\+\+INH&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_UM\_VOICE\_AMR\_RATSCCH\_MARKER@{GSMTAP\_UM\_VOICE\_AMR\_RATSCCH\_MARKER}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_UM\_VOICE\_AMR\_RATSCCH\_MARKER@{GSMTAP\_UM\_VOICE\_AMR\_RATSCCH\_MARKER}}}\mbox{\label{gsmtap_8h_a32746df3f332bb431908704613166fe9a97192c0e62aa851c72becb5b74f1489f}} 
GSMTAP\+\_\+\+UM\+\_\+\+VOICE\+\_\+\+AMR\+\_\+\+RATSCCH\+\_\+\+MARKER&\\
\hline

\raisebox{\heightof{T}}[0pt][0pt]{\index{GSMTAP\_UM\_VOICE\_AMR\_RATSCCH\_DATA@{GSMTAP\_UM\_VOICE\_AMR\_RATSCCH\_DATA}!gsmtap.h@{gsmtap.h}}\index{gsmtap.h@{gsmtap.h}!GSMTAP\_UM\_VOICE\_AMR\_RATSCCH\_DATA@{GSMTAP\_UM\_VOICE\_AMR\_RATSCCH\_DATA}}}\mbox{\label{gsmtap_8h_a32746df3f332bb431908704613166fe9a08626ffe1154345b8ae84d3be459e865}} 
GSMTAP\+\_\+\+UM\+\_\+\+VOICE\+\_\+\+AMR\+\_\+\+RATSCCH\+\_\+\+DATA&\\
\hline

\end{DoxyEnumFields}


\doxysubsection{Variable Documentation}
\mbox{\label{gsmtap_8h_abfa272885d73131c2dfbb14e7909a2d0}} 
\index{gsmtap.h@{gsmtap.h}!\_\_attribute\_\_@{\_\_attribute\_\_}}
\index{\_\_attribute\_\_@{\_\_attribute\_\_}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{\_\_attribute\_\_}
{\footnotesize\ttfamily enum \textbf{ gsmtap\+\_\+um\+\_\+voice\+\_\+type} \+\_\+\+\_\+attribute\+\_\+\+\_\+}

\mbox{\label{gsmtap_8h_a4222f9e79132af2040d0ccaa7aad0b47}} 
\index{gsmtap.h@{gsmtap.h}!\_pad@{\_pad}}
\index{\_pad@{\_pad}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{\_pad}
{\footnotesize\ttfamily uint8\+\_\+t \+\_\+pad[3]}

\mbox{\label{gsmtap_8h_ad8efa0c4c2acba3fa03a54b82ee8eeee}} 
\index{gsmtap.h@{gsmtap.h}!antenna\_nr@{antenna\_nr}}
\index{antenna\_nr@{antenna\_nr}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{antenna\_nr}
{\footnotesize\ttfamily uint8\+\_\+t antenna\+\_\+nr}



Antenna Number. 

\mbox{\label{gsmtap_8h_ae47d6bf4a702d6e5d0875693194d8373}} 
\index{gsmtap.h@{gsmtap.h}!arfcn@{arfcn}}
\index{arfcn@{arfcn}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{arfcn}
{\footnotesize\ttfamily uint16\+\_\+t arfcn}



ARFCN (frequency) 



Referenced by \textbf{ gsmtap\+\_\+makemsg()}, and \textbf{ gsmtap\+\_\+makemsg\+\_\+ex()}.

\mbox{\label{gsmtap_8h_a57cc7f4d579276167efca6cf047839b2}} 
\index{gsmtap.h@{gsmtap.h}!frame\_number@{frame\_number}}
\index{frame\_number@{frame\_number}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{frame\_number}
{\footnotesize\ttfamily uint32\+\_\+t frame\+\_\+number}



GSM Frame Number (FN) 

\mbox{\label{gsmtap_8h_adb7c2e546c05e4b147acd396ae594396}} 
\index{gsmtap.h@{gsmtap.h}!hdr\_len@{hdr\_len}}
\index{hdr\_len@{hdr\_len}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{hdr\_len}
{\footnotesize\ttfamily uint8\+\_\+t hdr\+\_\+len}



length in number of 32bit words 

\mbox{\label{gsmtap_8h_abbb6c7c49508c1ac374683f2d1159e08}} 
\index{gsmtap.h@{gsmtap.h}!level@{level}}
\index{level@{level}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{level}
{\footnotesize\ttfamily uint8\+\_\+t level}



logging level 



Referenced by \textbf{ \+\_\+file\+\_\+raw\+\_\+output()}, \textbf{ \+\_\+gsmtap\+\_\+raw\+\_\+output()}, \textbf{ \+\_\+msgb\+\_\+eq()}, \textbf{ \+\_\+osmo\+\_\+backtrace()}, \textbf{ \+\_\+output()}, \textbf{ \+\_\+output\+\_\+buf()}, \textbf{ \+\_\+systemd\+\_\+output()}, \textbf{ \+\_\+systemd\+\_\+raw\+\_\+output()}, \textbf{ level\+\_\+color()}, \textbf{ log\+\_\+cache\+\_\+check()}, \textbf{ log\+\_\+cache\+\_\+update()}, \textbf{ log\+\_\+check\+\_\+level()}, \textbf{ log\+\_\+parse\+\_\+category\+\_\+mask()}, \textbf{ log\+\_\+set\+\_\+category\+\_\+filter()}, \textbf{ logp2()}, \textbf{ logp2syslog\+\_\+level()}, \textbf{ osmo\+\_\+log\+\_\+backtrace()}, and \textbf{ osmo\+\_\+vlogp()}.

\mbox{\label{gsmtap_8h_ad086eea83d5646a9b756435887bf759d}} 
\index{gsmtap.h@{gsmtap.h}!line\_nr@{line\_nr}}
\index{line\_nr@{line\_nr}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{line\_nr}
{\footnotesize\ttfamily uint32\+\_\+t line\+\_\+nr}



line number 

\mbox{\label{gsmtap_8h_abc1e86d7c344fe34ff09e72d4595ab7e}} 
\index{gsmtap.h@{gsmtap.h}!name@{name}}
\index{name@{name}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{name}
{\footnotesize\ttfamily char name[32]}



source file name 

\mbox{\label{gsmtap_8h_aec32162d9dc3fde2c76d766af522dae5}} 
\index{gsmtap.h@{gsmtap.h}!pid@{pid}}
\index{pid@{pid}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{pid}
{\footnotesize\ttfamily uint32\+\_\+t pid}



process ID 



Referenced by \textbf{ osmo\+\_\+daemonize()}.

\mbox{\label{gsmtap_8h_a74d31d112440ebc015278c64cce0ed9e}} 
\index{gsmtap.h@{gsmtap.h}!proc\_name@{proc\_name}}
\index{proc\_name@{proc\_name}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{proc\_name}
{\footnotesize\ttfamily char proc\+\_\+name[16]}



name of process 

\mbox{\label{gsmtap_8h_a29850f3918435f089b2e206b9da59936}} 
\index{gsmtap.h@{gsmtap.h}!res@{res}}
\index{res@{res}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{res}
{\footnotesize\ttfamily uint8\+\_\+t res}



reserved for future use (RFU) 

\mbox{\label{gsmtap_8h_aaf5f5a3fa5d596a9136b4331f2b54bfc}} 
\index{gsmtap.h@{gsmtap.h}!sec@{sec}}
\index{sec@{sec}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{sec}
{\footnotesize\ttfamily uint32\+\_\+t sec}

\mbox{\label{gsmtap_8h_aede0b10bd33472950ab2153bb896817e}} 
\index{gsmtap.h@{gsmtap.h}!signal\_dbm@{signal\_dbm}}
\index{signal\_dbm@{signal\_dbm}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{signal\_dbm}
{\footnotesize\ttfamily int8\+\_\+t signal\+\_\+dbm}



signal level in d\+Bm 



Referenced by \textbf{ gsmtap\+\_\+makemsg()}, and \textbf{ gsmtap\+\_\+makemsg\+\_\+ex()}.

\mbox{\label{gsmtap_8h_a453ed986215416bdfd8502dd5a2b4910}} 
\index{gsmtap.h@{gsmtap.h}!snr\_db@{snr\_db}}
\index{snr\_db@{snr\_db}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{snr\_db}
{\footnotesize\ttfamily int8\+\_\+t snr\+\_\+db}



signal/noise ratio in dB 

\mbox{\label{gsmtap_8h_a2a6e4baad0b5d54944cc80100bdf7396}} 
\index{gsmtap.h@{gsmtap.h}!src\_file@{src\_file}}
\index{src\_file@{src\_file}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{}
{\footnotesize\ttfamily struct  \{ ... \}  src\+\_\+file}

\mbox{\label{gsmtap_8h_a29974f21be6fb35cb2b3c92f735b108f}} 
\index{gsmtap.h@{gsmtap.h}!sub\_slot@{sub\_slot}}
\index{sub\_slot@{sub\_slot}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{sub\_slot}
{\footnotesize\ttfamily uint8\+\_\+t sub\+\_\+slot}



sub-\/slot within timeslot 

\mbox{\label{gsmtap_8h_a1a2a5c6b28c6a619536d0b2250167609}} 
\index{gsmtap.h@{gsmtap.h}!sub\_type@{sub\_type}}
\index{sub\_type@{sub\_type}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{sub\_type}
{\footnotesize\ttfamily uint8\+\_\+t sub\+\_\+type}



Type of burst/channel, see above. 

\mbox{\label{gsmtap_8h_a0256c9929c7f63004cdcb9ee29f3ef13}} 
\index{gsmtap.h@{gsmtap.h}!subsys@{subsys}}
\index{subsys@{subsys}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{subsys}
{\footnotesize\ttfamily char subsys[16]}



logging sub-\/system 



Referenced by \textbf{ \+\_\+file\+\_\+raw\+\_\+output()}, \textbf{ \+\_\+gsmtap\+\_\+raw\+\_\+output()}, \textbf{ \+\_\+osmo\+\_\+backtrace()}, \textbf{ \+\_\+output()}, \textbf{ \+\_\+output\+\_\+buf()}, \textbf{ \+\_\+systemd\+\_\+raw\+\_\+output()}, \textbf{ color()}, \textbf{ log\+\_\+category\+\_\+name()}, \textbf{ log\+\_\+check\+\_\+level()}, \textbf{ logp()}, \textbf{ logp2()}, \textbf{ map\+\_\+subsys()}, \textbf{ osmo\+\_\+log\+\_\+backtrace()}, \textbf{ osmo\+\_\+signal\+\_\+dispatch()}, \textbf{ osmo\+\_\+signal\+\_\+register\+\_\+handler()}, \textbf{ osmo\+\_\+signal\+\_\+unregister\+\_\+handler()}, \textbf{ osmo\+\_\+vlogp()}, \textbf{ should\+\_\+log\+\_\+to\+\_\+target()}, and \textbf{ subsys\+\_\+lib2index()}.

\mbox{\label{gsmtap_8h_a37fa47dff193b952727a044c66718acf}} 
\index{gsmtap.h@{gsmtap.h}!timeslot@{timeslot}}
\index{timeslot@{timeslot}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{timeslot}
{\footnotesize\ttfamily uint8\+\_\+t timeslot}



timeslot (0..7 on Um) 

\mbox{\label{gsmtap_8h_aacc0eec328b2bbc6d4259c230516e609}} 
\index{gsmtap.h@{gsmtap.h}!ts@{ts}}
\index{ts@{ts}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{}
{\footnotesize\ttfamily struct  \{ ... \}  ts}



Referenced by \textbf{ gsmtap\+\_\+makemsg()}, and \textbf{ gsmtap\+\_\+makemsg\+\_\+ex()}.

\mbox{\label{gsmtap_8h_a1d127017fb298b889f4ba24752d08b8e}} 
\index{gsmtap.h@{gsmtap.h}!type@{type}}
\index{type@{type}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{type}
{\footnotesize\ttfamily uint8\+\_\+t type}



see GSMTAP\+\_\+\+TYPE\+\_\+$\ast$ 

\mbox{\label{gsmtap_8h_a400aa5c8c3b57ac30b6c9090f46cbdd7}} 
\index{gsmtap.h@{gsmtap.h}!usec@{usec}}
\index{usec@{usec}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{usec}
{\footnotesize\ttfamily uint32\+\_\+t usec}

\mbox{\label{gsmtap_8h_ab22abc2906422da61885ac6c8e6a1a59}} 
\index{gsmtap.h@{gsmtap.h}!version@{version}}
\index{version@{version}!gsmtap.h@{gsmtap.h}}
\doxysubsubsection{version}
{\footnotesize\ttfamily uint8\+\_\+t version}



version, set to 0x01 currently 

