\doxysection{osmo\+\_\+gad\+\_\+ell\+\_\+arc Struct Reference}
\label{structosmo__gad__ell__arc}\index{osmo\_gad\_ell\_arc@{osmo\_gad\_ell\_arc}}


{\ttfamily \#include $<$gad.\+h$>$}

\doxysubsection*{Data Fields}
\begin{DoxyCompactItemize}
\item 
int32\+\_\+t \textbf{ lat}
\begin{DoxyCompactList}\small\item\em latitude in micro degrees (degrees $\ast$ 1e6), -\/90\textquotesingle{}000\textquotesingle{}000 (S) . \end{DoxyCompactList}\item 
int32\+\_\+t \textbf{ lon}
\begin{DoxyCompactList}\small\item\em longitude in micro degrees (degrees $\ast$ 1e6), -\/180\textquotesingle{}000\textquotesingle{}000 (W) . \end{DoxyCompactList}\item 
uint32\+\_\+t \textbf{ inner\+\_\+r}
\begin{DoxyCompactList}\small\item\em inner circle radius in mm (m $\ast$ 1e3) \end{DoxyCompactList}\item 
uint32\+\_\+t \textbf{ unc\+\_\+r}
\begin{DoxyCompactList}\small\item\em Uncertainty circle radius in millimeters, 0 . \end{DoxyCompactList}\item 
uint16\+\_\+t \textbf{ ofs\+\_\+angle}
\begin{DoxyCompactList}\small\item\em Offset angle of first arc edge in degrees from North clockwise (eastwards), 0..359. \end{DoxyCompactList}\item 
uint16\+\_\+t \textbf{ incl\+\_\+angle}
\begin{DoxyCompactList}\small\item\em Included angle defining the angular width of the arc, in degrees clockwise, 1..360. \end{DoxyCompactList}\item 
uint8\+\_\+t \textbf{ confidence}
\begin{DoxyCompactList}\small\item\em Confidence in percent, 0 = no information, 1..100\%, 101..128 = no information. \end{DoxyCompactList}\end{DoxyCompactItemize}


\doxysubsection{Field Documentation}
\mbox{\label{structosmo__gad__ell__arc_a6b9b3b296a1578ab925c7fb0fac68058}} 
\index{osmo\_gad\_ell\_arc@{osmo\_gad\_ell\_arc}!confidence@{confidence}}
\index{confidence@{confidence}!osmo\_gad\_ell\_arc@{osmo\_gad\_ell\_arc}}
\doxysubsubsection{confidence}
{\footnotesize\ttfamily uint8\+\_\+t osmo\+\_\+gad\+\_\+ell\+\_\+arc\+::confidence}



Confidence in percent, 0 = no information, 1..100\%, 101..128 = no information. 

\mbox{\label{structosmo__gad__ell__arc_ae95e89e6838bc2153ba8efbc45ab7e02}} 
\index{osmo\_gad\_ell\_arc@{osmo\_gad\_ell\_arc}!incl\_angle@{incl\_angle}}
\index{incl\_angle@{incl\_angle}!osmo\_gad\_ell\_arc@{osmo\_gad\_ell\_arc}}
\doxysubsubsection{incl\_angle}
{\footnotesize\ttfamily uint16\+\_\+t osmo\+\_\+gad\+\_\+ell\+\_\+arc\+::incl\+\_\+angle}



Included angle defining the angular width of the arc, in degrees clockwise, 1..360. 

Angle is coded in increments of 2 degrees. \mbox{\label{structosmo__gad__ell__arc_adbbf330d68a6ba15a74f686781d19fdc}} 
\index{osmo\_gad\_ell\_arc@{osmo\_gad\_ell\_arc}!inner\_r@{inner\_r}}
\index{inner\_r@{inner\_r}!osmo\_gad\_ell\_arc@{osmo\_gad\_ell\_arc}}
\doxysubsubsection{inner\_r}
{\footnotesize\ttfamily uint32\+\_\+t osmo\+\_\+gad\+\_\+ell\+\_\+arc\+::inner\+\_\+r}



inner circle radius in mm (m $\ast$ 1e3) 

\mbox{\label{structosmo__gad__ell__arc_a843e657d989852f18863fc3a56729641}} 
\index{osmo\_gad\_ell\_arc@{osmo\_gad\_ell\_arc}!lat@{lat}}
\index{lat@{lat}!osmo\_gad\_ell\_arc@{osmo\_gad\_ell\_arc}}
\doxysubsubsection{lat}
{\footnotesize\ttfamily int32\+\_\+t osmo\+\_\+gad\+\_\+ell\+\_\+arc\+::lat}



latitude in micro degrees (degrees $\ast$ 1e6), -\/90\textquotesingle{}000\textquotesingle{}000 (S) . 

. 90\textquotesingle{}000\textquotesingle{}000 (N). \mbox{\label{structosmo__gad__ell__arc_abb328722fff32bf55d8f84596e086da8}} 
\index{osmo\_gad\_ell\_arc@{osmo\_gad\_ell\_arc}!lon@{lon}}
\index{lon@{lon}!osmo\_gad\_ell\_arc@{osmo\_gad\_ell\_arc}}
\doxysubsubsection{lon}
{\footnotesize\ttfamily int32\+\_\+t osmo\+\_\+gad\+\_\+ell\+\_\+arc\+::lon}



longitude in micro degrees (degrees $\ast$ 1e6), -\/180\textquotesingle{}000\textquotesingle{}000 (W) . 

. 180\textquotesingle{}000\textquotesingle{}000 (E). \mbox{\label{structosmo__gad__ell__arc_a48994910e4f32080f72c6e778a560f67}} 
\index{osmo\_gad\_ell\_arc@{osmo\_gad\_ell\_arc}!ofs\_angle@{ofs\_angle}}
\index{ofs\_angle@{ofs\_angle}!osmo\_gad\_ell\_arc@{osmo\_gad\_ell\_arc}}
\doxysubsubsection{ofs\_angle}
{\footnotesize\ttfamily uint16\+\_\+t osmo\+\_\+gad\+\_\+ell\+\_\+arc\+::ofs\+\_\+angle}



Offset angle of first arc edge in degrees from North clockwise (eastwards), 0..359. 

Angle is coded in increments of 2 degrees. \mbox{\label{structosmo__gad__ell__arc_a2f0540dfa7201d423fb2d6a3d6569c6e}} 
\index{osmo\_gad\_ell\_arc@{osmo\_gad\_ell\_arc}!unc\_r@{unc\_r}}
\index{unc\_r@{unc\_r}!osmo\_gad\_ell\_arc@{osmo\_gad\_ell\_arc}}
\doxysubsubsection{unc\_r}
{\footnotesize\ttfamily uint32\+\_\+t osmo\+\_\+gad\+\_\+ell\+\_\+arc\+::unc\+\_\+r}



Uncertainty circle radius in millimeters, 0 . 

. 18\textquotesingle{}000\textquotesingle{}000. Coding of uncertainty is non-\/linear, use osmo\+\_\+gad\+\_\+dec\+\_\+unc(osmo\+\_\+gad\+\_\+enc\+\_\+unc(val)) to clamp. 

The documentation for this struct was generated from the following file\+:\begin{DoxyCompactItemize}
\item 
include/osmocom/gsm/\textbf{ gad.\+h}\end{DoxyCompactItemize}
