\doxysection{ph\+\_\+tch\+\_\+param Struct Reference}
\label{structph__tch__param}\index{ph\_tch\_param@{ph\_tch\_param}}


for TCH.  




{\ttfamily \#include $<$l1sap.\+h$>$}

\doxysubsection*{Data Fields}
\begin{DoxyCompactItemize}
\item 
uint8\+\_\+t \textbf{ chan\+\_\+nr}
\begin{DoxyCompactList}\small\item\em Channel Number (Like RSL) \end{DoxyCompactList}\item 
uint32\+\_\+t \textbf{ fn}
\begin{DoxyCompactList}\small\item\em GSM Frame Number. \end{DoxyCompactList}\item 
int8\+\_\+t \textbf{ rssi}
\begin{DoxyCompactList}\small\item\em RSSI of received indication. \end{DoxyCompactList}\item 
uint8\+\_\+t \textbf{ marker}
\begin{DoxyCompactList}\small\item\em RTP Marker bit (speech onset indicator) \end{DoxyCompactList}\item 
uint16\+\_\+t \textbf{ ber10k}
\begin{DoxyCompactList}\small\item\em BER in units of 0.\+01\%. \end{DoxyCompactList}\item 
int16\+\_\+t \textbf{ lqual\+\_\+cb}
\begin{DoxyCompactList}\small\item\em Link quality in centi\+Bel. \end{DoxyCompactList}\item 
int16\+\_\+t \textbf{ ta\+\_\+offs\+\_\+256bits}
\begin{DoxyCompactList}\small\item\em timing advance offset (in 1/256th bits) \end{DoxyCompactList}\item 
uint8\+\_\+t \textbf{ is\+\_\+sub}\+:1
\begin{DoxyCompactList}\small\item\em flags \end{DoxyCompactList}\end{DoxyCompactItemize}


\doxysubsection{Detailed Description}
for TCH. 

\{req,ind\} $\vert$ TCH-\/\+RTS.\+ind 

\doxysubsection{Field Documentation}
\mbox{\label{structph__tch__param_a61f985800064f9fb098e3579fa0b9c39}} 
\index{ph\_tch\_param@{ph\_tch\_param}!ber10k@{ber10k}}
\index{ber10k@{ber10k}!ph\_tch\_param@{ph\_tch\_param}}
\doxysubsubsection{ber10k}
{\footnotesize\ttfamily uint16\+\_\+t ph\+\_\+tch\+\_\+param\+::ber10k}



BER in units of 0.\+01\%. 

\mbox{\label{structph__tch__param_a8ca8c93c07b134ff44f0c82d62afeab2}} 
\index{ph\_tch\_param@{ph\_tch\_param}!chan\_nr@{chan\_nr}}
\index{chan\_nr@{chan\_nr}!ph\_tch\_param@{ph\_tch\_param}}
\doxysubsubsection{chan\_nr}
{\footnotesize\ttfamily uint8\+\_\+t ph\+\_\+tch\+\_\+param\+::chan\+\_\+nr}



Channel Number (Like RSL) 

\mbox{\label{structph__tch__param_a66a0ccf020297591040f963ce1831933}} 
\index{ph\_tch\_param@{ph\_tch\_param}!fn@{fn}}
\index{fn@{fn}!ph\_tch\_param@{ph\_tch\_param}}
\doxysubsubsection{fn}
{\footnotesize\ttfamily uint32\+\_\+t ph\+\_\+tch\+\_\+param\+::fn}



GSM Frame Number. 

\mbox{\label{structph__tch__param_a7d36cc234a671a063e0ec7b4e93a323c}} 
\index{ph\_tch\_param@{ph\_tch\_param}!is\_sub@{is\_sub}}
\index{is\_sub@{is\_sub}!ph\_tch\_param@{ph\_tch\_param}}
\doxysubsubsection{is\_sub}
{\footnotesize\ttfamily uint8\+\_\+t ph\+\_\+tch\+\_\+param\+::is\+\_\+sub}



flags 

\mbox{\label{structph__tch__param_ab680e5beae92dd4be4f96b75dbc501a9}} 
\index{ph\_tch\_param@{ph\_tch\_param}!lqual\_cb@{lqual\_cb}}
\index{lqual\_cb@{lqual\_cb}!ph\_tch\_param@{ph\_tch\_param}}
\doxysubsubsection{lqual\_cb}
{\footnotesize\ttfamily int16\+\_\+t ph\+\_\+tch\+\_\+param\+::lqual\+\_\+cb}



Link quality in centi\+Bel. 

\mbox{\label{structph__tch__param_a7c92379d8c2e106ffc5d426f4dcf9578}} 
\index{ph\_tch\_param@{ph\_tch\_param}!marker@{marker}}
\index{marker@{marker}!ph\_tch\_param@{ph\_tch\_param}}
\doxysubsubsection{marker}
{\footnotesize\ttfamily uint8\+\_\+t ph\+\_\+tch\+\_\+param\+::marker}



RTP Marker bit (speech onset indicator) 

\mbox{\label{structph__tch__param_ab3f308c6282d3a1ff820fd656f591fd4}} 
\index{ph\_tch\_param@{ph\_tch\_param}!rssi@{rssi}}
\index{rssi@{rssi}!ph\_tch\_param@{ph\_tch\_param}}
\doxysubsubsection{rssi}
{\footnotesize\ttfamily int8\+\_\+t ph\+\_\+tch\+\_\+param\+::rssi}



RSSI of received indication. 

\mbox{\label{structph__tch__param_a59e8629f4cec5ac7022725c82d48c5ce}} 
\index{ph\_tch\_param@{ph\_tch\_param}!ta\_offs\_256bits@{ta\_offs\_256bits}}
\index{ta\_offs\_256bits@{ta\_offs\_256bits}!ph\_tch\_param@{ph\_tch\_param}}
\doxysubsubsection{ta\_offs\_256bits}
{\footnotesize\ttfamily int16\+\_\+t ph\+\_\+tch\+\_\+param\+::ta\+\_\+offs\+\_\+256bits}



timing advance offset (in 1/256th bits) 



The documentation for this struct was generated from the following file\+:\begin{DoxyCompactItemize}
\item 
include/osmocom/gsm/\textbf{ l1sap.\+h}\end{DoxyCompactItemize}
